|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Designation** | | **UM** | **Qty** |
| **PDR FOR UNIT: 500-PSV-1311** | | | | |
| **1** | **Spring  Model No.: BP513012BConst: Tyco** | | **ROOM** | **2** |
| **2** | **Seat  Model No.: BP513012BConst: Tyco** | | **ROOM** | **2** |
| **3** | **Disc  316SST Model No.: BP513012BConst: Tyco** | | **ROOM** | **2** |
| **PDR FOR UNIT: 500-PSV-1201/1202** | | | | |
| **4** | **Spring  N°18 on DrawingModel N°: 1E2 JBS-E-36-SPL-KConst: Tyco** | | **ROOM** | **2** |
| **5** | **Disc Insert  N°8 on DrawingModel N°: 1E2 JBS-E-36-SPL-KConst: Tyco** | | **ROOM** | **2** |
| **6** | **Disc Holder  N°5 on DrawingModel N°: 1E2 JBS-E-36-SPL-KConst: Tyco** | | **ROOM** | **2** |
| **7** | **Nozzle  N°2 on DrawingModel N°: 1E2 JBS-E-36-SPL-KConst: Tyco** | | **ROOM** | **2** |
| **PDR FOR UNIT: 200-PSV-2701/2706** | | | | |
| **8** | **Spring  Inlet 3/4''300RF Outlet: 1''300RFModel No.: 81PS1SB8B-4Const: Tyco** | | **ROOM** | **2** |
| **9** | **Disc Insert  Inlet 3/4''300RF Outlet: 1''300RFModel No.: 81PS1SB8B-4Const: Tyco** | | **ROOM** | **2** |
| **10** | **Spindle  Inlet 3/4''300RF Outlet: 1''300RFModel No.: 81PS1SB8B-4Const: Tyco** | | **ROOM** | **2** |
| **PDR FOR UNIT: 100-1080-1051-600-63-1031-11 PSV 81PS1S6B8A-SERIES 80** | | | | |
| **11** | **Seat  Model No.: 81PS1S6B8A-SERIE 80Const: Tyco** | | **ROOM** | **8** |
| **PDR FOR UNIT: 100-11-1082-10 PSV 44305T810/S1** | | | | |
| **12** | **Piston Seal  Model No.: 44305T810/S1Const: Tyco** | | **ROOM** | **6** |
| **13** | **Seat  Model No.: 44305T810/S1Const: Tyco** | | **ROOM** | **6** |
| **14** | **Linear seal  Model No.: 44305T810/S1Const: Tyco** | | **ROOM** | **6** |
| **15** | **Spring  Model No.: 44305T810/S1Const: Tyco** | | **ROOM** | **6** |
| **16** | **Disc Holder  Model No.: 44305T810/S1Const: Tyco** | | **ROOM** | **6** |
| **PDR FOR UNIT: 100-1080-1051-600-63-1031-11 PSV 81PS1S6B8A-SERIES 80** | | | | |
| **17** | **Spring  Model No.: 81PS1S6B8A-SERIE 80Const: Tyco** | | **ROOM** | **8** |
| **18** | **Spindle seal  Model No.: 81PS1S6B8A-SERIE 80Const: Tyco** | | **ROOM** | **8** |
| **19** | **Stabilizing ring  Model No.: 81PS1S6B8A-SERIE 80Const: Tyco** | | **ROOM** | **8** |
| **20** | **Spindle  Model No.: 81PS1S6B8A-SERIE 80Const: Tyco** | | **ROOM** | **8** |
| **21** | **Guide seal  Model No.: 81PS1S6B8A-SERIE 80Const: Tyco** | | **ROOM** | **8** |
| **22** | **Bushing seal  Model N°: 81PS1S6B8A-SERIE 80Const: Tyco** | | **ROOM** | **8** |
| **PDR FOR UNIT: 100-11-1082-10 PSV 3K4 JBS-E-15E** | | | | |
| **23** | **Bellows  Model No.: 3K4 JBS-E-15EConst: Tyco** | | **ROOM** | **6** |
| **24** | **Spring  Bellows Model No.: 3K4 JBS-E-15EConst: Tyco** | | **ROOM** | **6** |
| **25** | **Disc Holder  Bellows Model No.: 3K4 JBS-E-15EConst: Tyco** | | **ROOM** | **6** |
| **PDR FOR UNIT: 100-11-1082-10 PSV 1.5G3 JBS-E-15-K** | | | | |
| **26** | **Bellows  Model No.: 1.5G3 JBS-E-15-KConst: Tyco** | | **ROOM** | **6** |
| **PDR FOR UNIT: 100-11-1082-10 PSV 8T10 JBS-E-15-K** | | | | |
| **27** | **Disc Holder  Model No.: 8T10 JBS-E-15-KConst: Tyco** | | **ROOM** | **10** |
| **PDR FOR UNIT: 100-11-1082-10 PSV 8T10 JBS-E-45-K** | | | | |
| **28** | **Disc Holder  8T10 JBS-E-45-KConst: Tyco** | | **ROOM** | **6** |
| **PDR FOR PSV 900 SERIES VALVE MODEL 913BGF M06 JEO 145** | | | | |
| **29** | **Cap o-ring  N°23 on Drawing Valve PSV SERIE900 MODEL 913BGF M06 JEO 145Const: KUNKLE (TYCO)** | | **ROOM** | **10** |
| **30** | **Gag screw gasket  N°23 on Drawing PTFEValve PSV SERIE900 MODEL 913BGF M06 JEO 145Const: KUNKLE (TYCO)** | | **ROOM** | **10** |
| **31** | **Spring  Ref: SS A313-316 OR A313-T631/Alloy steel: A681-H12 OR B637-X750Const: KUNKLE (TYCO)** | | **ROOM** | **10** |
| **32** | **O-ring  cap N°12 on Drawing PTFEValve PSV SERIE900 MODEL 913BGF M06 JEO 145Const: KUNKLE (TYCO)** | | **ROOM** | **10** |
| **PDR FOR UNIT: 100-11-1082-10 PSV 6Q8 JBS-E-15-K** | | | | |
| **33** | **Bellows  Model No.: 6Q8 JBS-E-15-KConst: Tyco** | | **ROOM** | **6** |
| **PDR FOR PSV 900 SERIES VALVE MODEL 913BGF M06 JEO 145** | | | | |
| **34** | **O-ring body  N°02 on Drawing PTFEValve PSV SERIE900 MODEL 913BGF M06 JEO 145Const: KUNKLE (TYCO)** | | **ROOM** | **10** |
| **35** | **Disc  Ref: /SS A479-315N°05 on Drawing Valve PSV SERIE900 MODEL 913BGF M06 JEO 145Const: KUNKLE (TYCO)** | | **ROOM** | **10** |
| **36** | **Seal  N°02 on Drawing PTFEValve PSV SERIE900 MODEL 913BGF M06 JEO 145Const: KUNKLE (TYCO)** | | **ROOM** | **10** |
| **37** | **Disc Holder  Ref: BRASS,B16,(SS A351-CF8M Model913,919 ONLYValve PSV SERIE900 MODEL 913BGF M06 JEO 145Const: KUNKLE (TYCO)** | | **ROOM** | **10** |
| **PDR FOR UNIT: 100-1080-1051-600-63-1031-11 PSV 1.5H3 JOS-HE-15-C** | | | | |
| **38** | **Bellows  PSV Model No.: 1.5H3 JOS-HE-15-CConst: Tyco** | | **ROOM** | **6** |
| **39** | **Disc Insert  PSV Model No.: 1.5H3 JOS-HE-15-CConst: Tyco** | | **ROOM** | **6** |
| **40** | **Spring  PSV Model No.: 1.5H3 JOS-HE-15-CConst: Tyco** | | **ROOM** | **6** |
| **41** | **Disc holder  PSV Model No.: 1.5H3 JOS-HE-15-CConst: Tyco** | | **ROOM** | **6** |
| **42** | **o-ring kit  Model No.: 1.5H3 JOS-HE-15-CConst: Tyco** | | **ROOM** | **6** |
| **PDR FOR UNIT: 100-1080-1051-600-63-1031-11 PSV 81PS1S6B8A-SERIES 80** | | | | |
| **43** | **Blowdown adjustment screw seal  Model No.: 81PS1S6B8A-SERIE 80Const: Tyco** | | **ROOM** | **8** |
| **PDR FOR VALVE PSV 1D2 JOS-E35-K UNIT 700-701** | | | | |
| **44** | **Spring  Model No.: 1D2 JOS-E35-KConst: Tyco** | | **ROOM** | **6** |
| **PDR FOR UNIT: 100-11-1082-10 PSV 46305-1014/S1** | | | | |
| **45** | **Spring  PSV Model No.: 46305-1014/S1Const: Tyco** | | **ROOM** | **6** |
| **46** | **Disc holder  PSV Model No.: 46305-1014/S1Const: Tyco** | | **ROOM** | **6** |
| **47** | **Linear seal  PSV Model No.: 46305-1014/S1Const: Tyco** | | **ROOM** | **6** |
| **48** | **Seat  Model No.: 46305-1014/S1Const: Tyco** | | **ROOM** | **6** |
| **49** | **Piston Seal  PSV Model No.: 46305-1014/S1Const: Tyco** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 1E2 JOS-E35-N2-K UNIT 700-701** | | | | |
| **50** | **Spring  Model No.: 1E2 JOS-E35-N2-KConst: Tyco** | | **ROOM** | **6** |
| **PDR FOR UNIT: 100-1080-1051-600-63-1031-11 PSV 6Q8 JBS-E-35-K** | | | | |
| **51** | **O-ring kit  Model No.: 6Q8 JBS-E-35-KConst: Tyco** | | **ROOM** | **6** |
| **52** | **Disc holder  PSV Model No.: 6Q8 JBS-E-35-KConst: Tyco** | | **ROOM** | **6** |
| **53** | **Spring  Model No.: 6Q8 JBS-E-35-KConst: Tyco** | | **ROOM** | **6** |
| **54** | **Bellows  PSV Model No.: 6Q8 JBS-E-35-KConst: Tyco** | | **ROOM** | **6** |
| **PDR FOR UNIT: 700-701-11-1051-1071-1061-1031-1081-31-1082-1060-100** | | | | |
| **55** | **Disc insert  Part N° 145873Model N°: 6R10 JOSH-E & JBS-EConst: Tyco** | | **ROOM** | **10** |
| **PDR FOR UNIT: 900-PSV-1401/1402** | | | | |
| **56** | **Spring for PSV  CRM STL/1215 STLPart No. SX36026-103200Model No.: 1D2 JBS-E-35-KConst: Tyco** | | **ROOM** | **2** |
| **57** | **Disc insert for PSV  SST SAA479-316Part No. 136977Model No.: 1D2 JBS-E-35-KConst: Tyco** | | **ROOM** | **2** |
| **58** | **Disc holder for PSV  SST SAA479-316LPart No. 147151Model No.: 1D2 JBS-E-35-KConst: Tyco** | | **ROOM** | **2** |
| **59** | **Nozzle for PSV  SST SA351-CF8MSST SAA479-316Part No. 103185Model No.: 1D2 JBS-E-35-KConst: Tyco** | | **ROOM** | **2** |
| **PDR FOR UNIT: 500-PSV-5501/900-PSV-1101A/B** | | | | |
| **60** | **Spring for PSV  Inconel X-750Model No: 1E2 JBS-E-16-KConst: Tyco** | | **ROOM** | **3** |
| **61** | **Disc insert for PSV  ASME SA479TYPE 316Model No: 1E2 JBS-E-16-KConst: Tyco** | | **ROOM** | **3** |
| **62** | **Disc holder for PSV  316 L SST Model No.: 1E2 JBS-E-16-KConst: Tyco** | | **ROOM** | **3** |
| **63** | **Nozzle for PSV  ASME SA351 GR CF8M Model No.: 1E2 JBS-E-16-KConst: Tyco** | | **ROOM** | **3** |
| **PDR FOR UNIT: 500-PSV-1901** | | | | |
| **64** | **Spring for PSV  CRM STL/1215 STLPart No. SX36076-102713Model No.: 1.5G3 JIS-HE-15-CConst: Tyco** | | **ROOM** | **2** |
| **65** | **Disc insert for PSV  SST SA479-315Part No. 136979Model No.: 1.5G3 JIS-HE-15-CConst: Tyco** | | **ROOM** | **2** |
| **66** | **Disc holder for PSV  SST SA351-CF3MPart No. 147156Model No.: 1.5G3 JIS-HE-15-CConst: Tyco** | | **ROOM** | **2** |
| **67** | **Nozzle for PSV  SST SA351-CF8MPart No. 102813Model No.: 1.5G3 JIS-HE-15-CConst: Tyco** | | **ROOM** | **2** |
| **PDR FOR UNIT: 500-PSV-1702** | | | | |
| **68** | **Spring for PSV  Model No.: 9511X12E-SPLConst: Tyco** | | **ROOM** | **2** |
| **69** | **Seat for PSV  Model No.: 9511X12E-SPLConst: Tyco** | | **ROOM** | **2** |
| **70** | **Disc for PSV  Model No.: 9511X12E-SPLConst: Tyco** | | **ROOM** | **2** |
| **PDR FOR UNIT: 500-PSV-1603A/B** | | | | |
| **71** | **Spring for PSV  Model No.: 1D2 JBS-E-25X-K-SPL-SPLConst: Tyco** | | **ROOM** | **2** |
| **72** | **Seat for PSV  Model No.: 1D2 JBS-E-25X-K-SPL-SPLConst: Tyco** | | **ROOM** | **2** |
| **73** | **Disc for PSV  Model No.: 1D2 JBS-E-25X-K-SPL-SPLConst: Tyco** | | **ROOM** | **2** |
| **PDR FOR UNIT: 500-PSV-1601A/B** | | | | |
| **74** | **Spring for PSV  No. 18 on drawingModel No.: 8T10 JBS-E-35-KConst: Tyco** | | **ROOM** | **2** |
| **75** | **Disc insert for PSV  N° 08 on drawingModel N°: 8T10 JBS-E-35-KConst: Tyco** | | **ROOM** | **2** |
| **76** | **Disc holder for PSV  No. 05 on drawingModel No.: 8T10 JBS-E-35-KConst: Tyco** | | **ROOM** | **2** |
| **77** | **Nozzle for PSV  N° 02 on drawingModel N°: 8T10 JBS-E-35-KConst: Tyco** | | **ROOM** | **2** |
| **PDR FOR UNIT: 700-701-11-1051-1071-1061-1031-1081-31-1082-1060-100** | | | | |
| **78** | **Spring  Part No. SX36375 Model No.: 8T10 JOS-HE-35-CConst: Tyco** | | **ROOM** | **10** |
| **79** | **Spring  Part No. SX36373 Model No.: 8T10 JBS-E-15-KConst: Tyco** | | **ROOM** | **10** |
| **80** | **Spring  Part No. SX36077 Model No.: 1.5H3 JLT-JBS-E-15-KConst: Tyco** | | **ROOM** | **10** |
| **81** | **Spring  Part No. SX36073 Model No.: 1.5H2 JLT-JBS-E-15-KConst: Tyco** | | **ROOM** | **10** |
| **82** | **Spring  Part No. SX36031 Model No.: 1D JOS-E-35-KConst: Tyco** | | **ROOM** | **10** |
| **83** | **Spring  Part No. SX36308 Model No.: 6Q8 JBS-E-35-KConst: Tyco** | | **ROOM** | **10** |
| **84** | **Spring  Part No. SX36156 Model No.: 3K4 JBS-E-OR-35-KConst: Tyco** | | **ROOM** | **10** |
| **85** | **Spring  Part No. SX36380 Model No.: 8T10 JOS-HE-45-CConst: Tyco** | | **ROOM** | **10** |
| **86** | **Spring  Part No. SX36375 Model No.: 8T10 JOS-HE-35-CConst: Tyco** | | **ROOM** | **10** |
| **87** | **Spring  Part No. SX36374 Model No.: 8T10 JOS-HE-35-CConst: Tyco** | | **ROOM** | **10** |
| **PDR FOR VALVE PSV 4L6 JOS-E35-N2-K UNIT: 700-701** | | | | |
| **88** | **Spring  Model No.: 4L6 JOS-E35-N2-KConst: Tyco** | | **ROOM** | **6** |
| **89** | **Disc holder  Model No.: 4L6 JOS-E35-N2-KConst: Tyco** | | **ROOM** | **6** |
| **90** | **O-ring kit  Model No.: 4L6 JOS-E35-N2-KConst: Tyco** | | **ROOM** | **6** |
| **PDR FOR UNIT: 100-11-1051-1082-10 PSV 46305-1014/S1** | | | | |
| **91** | **O-ring kit  Model No: 46305-1014/S1 Const: Tyco** | | **ROOM** | **6** |
| **PDR FOR PSV VALVE MODEL 26305-810/S1 UNIT 1070-1051-701** | | | | |
| **92** | **Bonnet seat  MODEL PSV 26305-810/S1N°08 on drawingConst: Tyco** | | **ROOM** | **6** |
| **93** | **Seat  MODEL PSV 26305-810/S1N°04 on drawingConst: Tyco** | | **ROOM** | **6** |
| **94** | **Nozzle seat  MODEL PSV 26305-810/S1N°02 on drawingConst: Tyco** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV MODEL 8T210 JOS-HE-15-C-SPL UNIT 1070-1051-701** | | | | |
| **95** | **Disc holder  MODEL PSV 8T210 JOS-HE-15-C-SPLConst: Tyco** | | **ROOM** | **6** |
| **FOR 400-PSV-1903A-1903B/2003A/2003B/2103A/2103B/400-PSV-2203A-2203B/2303A/2303B/2403A/2403B** | | | | |
| **96** | **Spring  MODEL PSV 3K4 JBS-E22-KS/N: 11-06811-06812Inlet: 3''300RFOutlet: 4''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **3** |
| **FOR 400-PSV-3503A/3503B 400-PSV-3603A-3603B** | | | | |
| **97** | **Disc insert  MODEL PSV 3K4 JBS-E25-S-KS/N: 11-06877-11-06878Inlet: 3''300RFOutlet: 4''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **98** | **Spring  MODEL PSV 3K4 JBS-E25-S-KS/N: 11-06877-11-06878Inlet: 3''300RFOutlet: 4''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **99** | **Disc holder  MODEL PSV 3K4 JBS-E25-S-KS/N: 11-06877-11-06878Inlet: 3''300RFOutlet: 4''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **100** | **Bellows  MODEL PSV 3K4 JBS-E25-S-KS/N: 11-06877-11-06878Inlet: 3''300RFOutlet: 4''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **101** | **Gasket kit  MODEL PSV 3K4 JBS-E25-S-KS/N: 11-06877-11-06878Inlet: 3''300RFOutlet: 4''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **FOR 200-PSV-1202/1203 200-PSV-1502/2303 400-PSV-1210** | | | | |
| **102** | **Disc insert  MODEL PSV 9511012E-25-STMS/N: 11-06789Inlet: 3/4''300RFOutlet: 1''150RF set pressure: 35KG/CM2G** | | **ROOM** | **2** |
| **103** | **Spring  MODEL PSV 9511012E-25-STMS/N: 11-06789Inlet: 3/4''300RFOutlet: 1''150RF set pressure: 35KG/CM2G** | | **ROOM** | **2** |
| **104** | **O.ring kit  MODEL PSV 9511012E-25-STMS/N: 11-06789Inlet: 3/4''300RFOutlet: 1''150RF set pressure: 35KG/CM2G** | | **ROOM** | **2** |
| **105** | **Disc holder  MODEL PSV 9511012E-25-STMS/N: 11-06789Inlet: 3/4''300RFOutlet: 1''150RF set pressure: 35KG/CM2G** | | **ROOM** | **2** |
| **FOR 400-PSV-4201A/4201B** | | | | |
| **106** | **Disc insert  MODEL PSV 1E2 JBS-E-15-KS/N: 11-06891-11-06892Inlet: 1''150RFOutlet: 2''150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **107** | **Spring  MODEL PSV 1E2 JBS-E-15-KS/N: 11-06891-11-06892Inlet: 1''150RFOutlet: 2''150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **108** | **Gasket kit  MODEL PSV 1E2 JBS-E-15-KS/N: 11-06891-11-06892Inlet: 1''150RFOutlet: 2''150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **109** | **Bellows tailpiece  MODEL PSV 1E2 JBS-E-15-KS/N: 11-06891-11-06892Inlet: 1''150RFOutlet: 2''150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **110** | **Disc holder  MODEL PSV 1E2 JBS-E-15-KS/N: 11-06891-11-06892Inlet: 1''150RFOutlet: 2''150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **FOR 400-PSV-1207/3302/3303 600-PSV-6802** | | | | |
| **111** | **Disc insert  MODEL PSV BP513011BS/N: 11-06786Inlet: 0.75''150RFOutlet: 1.5''150RF set pressure: 13.5KG/CM2G** | | **ROOM** | **2** |
| **112** | **O.ring kit  MODEL PSV BP513011BS/N: 11-06786Inlet: 0,75''150RFOutlet: 1,5''150RF set pressure: 13.5KG/CM2G** | | **ROOM** | **2** |
| **113** | **Spring  MODEL PSV BP513011BS/N: 11-06786Inlet: 0.75''150RFOutlet: 1.5''150RF set pressure: 13.5KG/CM2G** | | **ROOM** | **2** |
| **114** | **Disc holder  MODEL PSV BP513011BS/N: 11-06786Inlet: 0.75''150RFOutlet: 1.5''150RF set pressure: 13.5KG/CM2G** | | **ROOM** | **2** |
| **FOR 400-PSV-1603A/1603B/1603C** | | | | |
| **115** | **Disc insert  MODEL PSV BP513011BS/N: 11-06790-1106792Inlet: 0.75''150RFOutlet: 1''150RF set pressure: 9.5KG/CM2G** | | **ROOM** | **2** |
| **116** | **Spring  MODEL PSV BP513011BS/N: 11-06790-1106792Inlet: 0.75''150RFOutlet: 1''150RF set pressure: 9.5KG/CM2G** | | **ROOM** | **2** |
| **117** | **O.ring kit  MODEL PSV BP513011BS/N: 11-06790-1106792  Inlet: 0.75''150RF  Outlet: 1''150RF set pressure: 9.5KG/CM2G** | | **ROOM** | **2** |
| **118** | **Disc Holder  MODEL PSV BP513011BS/N: 11-06790-1106792Inlet: 0.75''150RFOutlet: 1''150RF set pressure: 9.5KG/CM2G** | | **ROOM** | **2** |
| **FOR 400-PSV-1801A-1801B** | | | | |
| **119** | **Disc Insert  MODEL PSV 1.5G3 JBS-E32-KS/N: 11-06805-11-0680Inlet: 1.5''150RFOutlet: 3''150RF set pressure: 16KG/CM2G** | | **ROOM** | **2** |
| **120** | **Spring  MODEL PSV 1.5G3 JBS-E32-KS/N: 11-06805-11-0680Inlet: 1.5''150RFOutlet: 3''150RF set pressure: 16KG/CM2G** | | **ROOM** | **2** |
| **121** | **Gasket kit  MODEL PSV 1.5G3 JBS-E32-KS/N: 11-06805-11-0680Inlet: 1,5''150RFOutlet: 3''150RF set pressure: 16KG/CM2G** | | **ROOM** | **2** |
| **122** | **Bellows tailpiece  MODEL PSV 1.5G3 JBS-E32-KS/N: 11-06805-11-0680Inlet: 1.5''150RFOutlet: 3''150RF set pressure: 16KG/CM2G** | | **ROOM** | **2** |
| **FOR 400-PSV-1901A-1901B/2001A/2001B/2101A/2101B - 400-PSV-2201A-2201B/2301A/2301B/2401A/2401B** | | | | |
| **123** | **Disc insert  MODEL PSV 3K4 JBS-E12-KS/N: 11-06807-11-06808Inlet: 3''150RFOutlet: 4''150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **3** |
| **124** | **Spring  MODEL PSV 3K4 JBS-E12-KS/N: 11-06807-11-06808Inlet: 3''150RFOutlet: 4''150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **3** |
| **125** | **Disc holder  MODEL PSV 3K4 JBS-E12-KS/N: 11-06807-11-06808Inlet: 3''150RFOutlet: 4''150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **3** |
| **126** | **Bellows  MODEL PSV 3K4 JBS-E12-KS/N: 11-06807-11-06808Inlet: 3''150RFOutlet: 4''150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **3** |
| **127** | **Gasket kit  MODEL PSV 3K4 JBS-E12-KS/N: 11-06807-11-06808Inlet: 3''150RFOutlet: 4''150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **3** |
| **FOR 400-PSV-1902A-1902B** | | | | |
| **128** | **Disc insert  MODEL PSV 1.5 JBS-E22-K-SPLS/N: 11-06809-11-06810Inlet: 1.5''150RFOutlet: 3''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **129** | **Spring  MODEL PSV 1.5 JBS-E22-K-SPLS/N: 11-06809-11-06810Inlet: 1.5''150RFOutlet: 3''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **130** | **Disc holder  MODEL PSV 1.5 JBS-E22-K-SPLS/N: 11-06809-11-06810Inlet: 1.5''150RFOutlet: 3''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **131** | **Bellows  MODEL PSV 1.5 JBS-E22-K-SPLS/N: 11-06809-11-06810Inlet: 1.5''150RFOutlet: 3''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **132** | **Gasket kit  MODEL PSV 1.5 JBS-E22-K-SPLS/N: 11-06809-11-06810Inlet: 1.5''150RFOutlet: 3''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **PDR FOR VALVE PSV 44310T810/S1 UNIT:701-103-1091** | | | | |
| **133** | **Piston seat  MODEL PSV N°: 44310T810/S1Const: TYCO** | | **ROOM** | **6** |
| **134** | **Seat  MODEL PSV No: 44310T810/S1 Const: TYCO** | | **ROOM** | **6** |
| **135** | **Linear seat  MODEL PSV N°: 44310T810/S1Const: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 1,5H3 -JBS-E-15-K UNIT:701-103-1091** | | | | |
| **136** | **Disc holder  MODEL PSV No.: 1.5H3 -JBS-E-15-K Const: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 1.5H3 JLT-E-15-E UNIT:701-103-1091** | | | | |
| **137** | **Disc holder  MODEL PSV No.: 1.5H3 JLT-E-15-EConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 1,5F2 JLT-JOS-E-36-K UNIT:31-11-10-700** | | | | |
| **138** | **Disc holder  MODEL PSV No.: 1.5F2 JLT-JOS-E-36-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 1,5G3 JLT-JOS-E-15-K UNIT:31-11-10-700** | | | | |
| **139** | **Disc holder  MODEL PSV No.: 1.5G3 JLT-JOS-E-15-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 6Q8 JBS-E-16-K UNIT:31-11-10-700** | | | | |
| **140** | **Disc holder  MODEL PSV N°: 6Q8 JBS-E-16-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 2J3 JBS-E-15-K UNIT:31-11-10-700** | | | | |
| **141** | **Disc holder  MODEL PSV No.: 2J3 JBS-E-15-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 4P6 JLT-JBS-E-15-K UNIT:31-11-10-700** | | | | |
| **142** | **Disc holder  MODEL PSV N°: JLT-JBS-E-15-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 1D2 JLT-JOS-E-35-K UNIT:31-11-10-700** | | | | |
| **143** | **Disc holder  MODEL PSV N°: 1D2 JLT-JOS-E-35-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 3K4 JBS-E-15-E UNIT:31-11-10-700** | | | | |
| **144** | **Disc holder  MODEL PSV N°: 3K4 JBS-E-15-EConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR PSV VALVE 1.5H JLT-JBS-E-15-K UNIT:31-11-10-700** | | | | |
| **145** | **Disc holder  MODEL PSV No.: 1.5H JLT-JBS-E-15-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 2J3 JOS-E-15-E UNIT:1081-700-701-100** | | | | |
| **146** | **Disc holder  MODEL PSV N°: 2J3 JOS-E-15-EConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 3L4 JOS-E-15-E UNIT:1081-700-701-100** | | | | |
| **147** | **Disc insert  MODEL PSV No.: 3L4 JOS-E-15-EConst: TYCO** | | **ROOM** | **6** |
| **148** | **O-ring  MODEL PSV N°: 3L4 JOS-E-15-EConst: TYCO** | | **ROOM** | **6** |
| **149** | **Cap gasket  MODEL PSV N°: 3L4 JOS-E-15-EConst: TYCO** | | **ROOM** | **6** |
| **150** | **Gasket guide  MODEL PSV N°: 3L4 JOS-E-15-EConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 8T10 JOS-HE-45-C UNIT:1070-1051-701** | | | | |
| **151** | **Disc holder  MODEL PSV N°: 8T10 JOS-HE-45-CConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 8T210 JOS-HE-15-C-SPL UNIT:1070-1051-701** | | | | |
| **152** | **Disc insert  MODEL PSV N°: 8T210 JOS-HE-15-C-SPLConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR PSV VALVE P/UNITE:10-11-100-30-31-200-1120-1121-1060-1070-400-500-900-700-701-702-703-1082-1081-62** | | | | |
| **153** | **Bellows  Part No: S91328MODEL: 2J3 JBS-E-15-K/E-12-EConst: TYCO** | | **ROOM** | **10** |
| **154** | **Bellows  Part No: S91326MODEL: 1.5G3 JBS-E-25-KConst: TYCO** | | **ROOM** | **10** |
| **155** | **Bellows  Part No: S91772MODEL: 6Q8 JBS-E-16-K/E-35-KConst: TYCO** | | **ROOM** | **10** |
| **156** | **Bellows  Part No: S91341MODEL: 8T10 JBS-E-45-KConst: TYCO** | | **ROOM** | **10** |
| **157** | **Bellows  Part No: S91741MODEL: 1.5H3 JLT-JBS-E-15-K and JBS-EConst: TYCO** | | **ROOM** | **10** |
| **PDR FOR VALVE PSV MODEL 1E2 JOS-E-35-K UNIT:1070-1051-701** | | | | |
| **158** | **Disc holder  MODEL PSV 1E2 JOS-E-35-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR PSV VALVE MODEL 26305-810/S1 UNIT:1070-1051-701** | | | | |
| **159** | **Blowdown seal  MODEL PSV 26305-810/S1N°24 on drawingConst: TYCO** | | **ROOM** | **6** |
| **160** | **Bushing seal  MODEL PSV 26305-810/S1N°21 on drawingConst: TYCO** | | **ROOM** | **6** |
| **161** | **Piston seal  MODEL PSV 26305-810/S1N°18 on drawingConst: TYCO** | | **ROOM** | **6** |
| **162** | **Blowdown  MODEL PSV 26305-810/S1N°16 on drawingConst: TYCO** | | **ROOM** | **6** |
| **163** | **Spring  MODEL PSV 26305-810/S1N°10 on drawingConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR UNIT: 700-701-11-1051-1071-1061-1031-1081-31-1082-1060-100** | | | | |
| **164** | **Spring  Part No.SX36372Model No.: 8T10 JBS-E-45-KConst: TYCO** | | **ROOM** | **10** |
| **PDR FOR UNIT: 100-11-1082-10 PSV 44305T810/S1** | | | | |
| **165** | **O-ring kit  Model No.: 44305T810/S1Const: TYCO** | | **ROOM** | **6** |
| **FOR 400-PSV-3502A/3502B** | | | | |
| **166** | **Disc holder  For PSV Model: 1.5G3 JBS-E-35-S-KS/N: 11-06875-1106876Inlet: 1.5'' 300RFOutlet: 3'' 150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **167** | **Disc insert  For PSV Model: 1.5G3 JBS-E-35-S-KS/N: 11-06875-1106876Inlet: 1.5'' 300RFOutlet: 3'' 150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **168** | **Spring  For PSV Model: 1.5G3 JBS-E-35-S-KS/N: 11-06875-1106876Inlet: 1.5'' 300RFOutlet: 3'' 150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **169** | **Gasket kit  For PSV Model: 1.5G3 JBS-E-35-S-KS/N: 11-06875-1106876Inlet: 1.5'' 300RFOutlet: 3'' 150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **170** | **Bellows  For PSV Model: 1.5G3 JBS-E-35-S-KS/N: 11-06875-1106876  Inlet: 1.5'' 300RF  Outlet: 3'' 150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **For 100-PSV-2201200-PSV-1801A/1801B 400-PSV-3401A-3401/B 701-PSv-1101A/1101B 703-PSV-1101A** | | | | |
| **171** | **Disc insert  For PSV Model: 3L4 JBS-E-15-S-KS/N: 11-06875-1106872Inlet: 3'' 300RFOutlet: 4'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **3** |
| **172** | **Spring  For PSV Model: 3L4 JBS-E-15-S-KS/N: 11-06875-1106872Inlet: 3'' 300RFOutlet: 4'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **3** |
| **FOR 400-PSV-2801A/2801B** | | | | |
| **173** | **Disc insert  For PSV Model: 4M6 JBS-E-12-KS/N: 11-06853-11-06854Inlet: 4'' 300RFOutlet: 6'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **174** | **Spring  For PSV Model: 4M6 JBS-E-12-KS/N: 11-06853-11-06854Inlet: 4'' 300RFOutlet: 6'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **175** | **Disc holder  For PSV Model: 4M6 JBS-E-12-KS/N: 11-06853-11-06854Inlet: 4'' 300RFOutlet: 6'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **176** | **Spindle  For PSV Model: 4M6 JBS-E-12-KS/N: 11-06853-11-06854Inlet: 4'' 300RFOutlet: 6'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **FOR 400-PSV-3101A/3102A 400-PSV-3001A/3001B** | | | | |
| **177** | **Spring  For PSV Model: 2J3 JBS-E-12-KS/N: 11-06862Inlet: 2'' 150RFOutlet: 3'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **178** | **Disc holder  For PSV Model: 2J3 JBS-E-12-KS/N: 11-06862Inlet: 2'' 150RFOutlet: 3'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **179** | **Spindle  For PSV Model: 2J3 JBS-E-12-KS/N: 11-06862Inlet: 2'' 150RFOutlet: 3'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **180** | **Disc insert  For PSV Model: 2J3 JBS-E-12-KS/N: 11-06862Inlet: 2'' 150RFOutlet: 3'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **FOR 400-PSV-3101A/3101A 400-PSV-3002A/3002B** | | | | |
| **181** | **Disc holder  For PSV Model: 56605-810/S1S/N: 11-06793-11-06796Inlet: 8'' 150RFOutlet: 10'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **FOR 10-PSV-1114/11-PSV-2114 100-PSv-2401A/2401B 400-PSV-3801A/3801B/3802A** | | | | |
| **182** | **Disc insert  For PSV Model: 2J3 JBS-E-15-KS/N: 11-06887-11-06888Inlet: 2'' 150RFOutlet: 3'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **3** |
| **183** | **Spring  For PSV Model: 2J3 JBS-E-15-KS/N: 11-06887-11-06888Inlet: 2'' 150RFOutlet: 3'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **3** |
| **184** | **Disc holder  For PSV Model: 2J3 JBS-E-15-KS/N: 11-06887-11-06888Inlet: 2'' 150RFOutlet: 3'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **3** |
| **PDR for unit: 200-PSV-1501A/B** | | | | |
| **185** | **Spring: SST 316  For PSV: 6" inlet 150RF OUTLET: 8" 150RFModel: 950608RS** | | **ROOM** | **2** |
| **186** | **Nozzle: SST SA479-316  For PSV: 6" inlet 150RF OUTLET: 8" 150RFModel: 950608RS** | | **ROOM** | **2** |
| **187** | **Spindle: SST SA479-304  For PSV: 6" inlet 150RF OUTLET: 8" 150RFModel: 950608RS** | | **ROOM** | **2** |
| **PDR for unit: 200-PSV-1204** | | | | |
| **188** | **Spring (KIT)  For PSV: 4" inlet 300RF OUTLET: 6" 150RFModel: 4N6 JLT-JBS-E-25-K- Part N°:SX36267-103157** | | **ROOM** | **1** |
| **189** | **Disc Insert: SST SA479-316  For PSV: 4" 300RF inlet OUTLET: 6" 150RFModel: 4N6 JLT-JBS-E-25-K Part N°: 145870** | | **ROOM** | **1** |
| **190** | **Disc Holder: SST SA351-CF3M  For PSV: 4" inlet 300RF OUTLET: 6" 150RFModel: 4N6 JLT-JBS-E-25-K Part N°: 146384** | | **ROOM** | **1** |
| **PDR for unit: 200-PSV-1101A/B** | | | | |
| **191** | **Disc Insert: SST SA479-316  For PSV: 3/4" inlet 150RF OUTLET: 1" 150RFModel: BP513011EPart N°: 122598** | | **ROOM** | **2** |
| **192** | **Disc Holder: SST SA479-316  For PSV: 3/4" inlet 150RF OUTLET: 1" 150RFModel: BP513011E Part N°: 140945** | | **ROOM** | **2** |
| **PDR for unit: 200-PSV-1902A/B** | | | | |
| **193** | **Spring (200-PSV-1101A,SN:06457)  For PSV: 3/4" inlet 150RF OUTLET: 1" 150RFModel: BP513011EPart N°: X09835** | | **ROOM** | **2** |
| **194** | **Spring (KIT)  For PSV: 1.5" inlet 150RF OUTLET: 3" 150RFModel: 1.5H3 JBS-E-15-E Part N°:SX36073-102713** | | **ROOM** | **2** |
| **195** | **Disc Insert: SST SA479-316  For PSV: 1.5" inlet 150RF OUTLET: 3" 150RFModel: 1.5H3 JBS-E-15-E Part N°: 136980** | | **ROOM** | **2** |
| **196** | **Disc Holder: SST SA351-CF3M  For PSV: 1.5" inlet 150RF OUTLET: 3" 150RFModel: 1.5H3 JBS-E-15-E Part N°: 147195** | | **ROOM** | **2** |
| **PDR for unit: 200-PSV-1901A/B** | | | | |
| **197** | **Spring (KIT)  For PSV: inlet 4" 150RF OUTLET: 6" 150RFModel: 4M6 JBS-E-15-E** | | **ROOM** | **2** |
| **198** | **Disc Insert: SST SA479-316  For PSV: 4" 150RF inlet OUTLET: 6" 150RFModel: 4M6 JBS-E-15-E** | | **ROOM** | **2** |
| **199** | **Disc Holder: SST SA351-CF3M  For PSV: 4" inlet 150RF OUTLET: 6" 150RFModel: 4M6 JBS-E-15-E** | | **ROOM** | **2** |
| **PDR for unit: 200-PSV-3002** | | | | |
| **200** | **Spring: Chrome steel  For PSV: inlet 6" 600RF OUTLET: 8" 150RFModel: 6Q8 JOS-HE-45-C** | | **ROOM** | **1** |
| **201** | **Disc Insert: ASME SA479  Type: 316For PSV: 6" 600RF inlet OUTLET: 6" 150RFModel: 6Q8 JOS-HE-45-C** | | **ROOM** | **1** |
| **202** | **Sprindle: 416 SST  For PSV: 6" inlet 600RF OUTLET: 8" 150RFModel: 6Q8 JOS-HE-45-C** | | **ROOM** | **1** |
| **PDR for unit: 200-PSV-2002A/2001A/2001B** | | | | |
| **203** | **Spring steel  For PSV: inlet 3" 300RF OUTLET: 4" 150RFModel: 3K4 JBS-E36-SPL TYPE K** | | **ROOM** | **3** |
| **204** | **Disc Insert: ASME SA479  Type: 316For PSV: 3" 300RF inlet OUTLET: 4" 150RFModel: 3K4 JBS-E36-SPL TYPE K** | | **ROOM** | **3** |
| **205** | **Disc Holder: 316L SST  For PSV: 3" 300RF inlet OUTLET: 4" 150RFModel: 3K4 JBS-E36-SPL TYPE K** | | **ROOM** | **3** |
| **PDR for PSV valve FOR unit: 10-11-100-30-31-200-1120-1121-1060-170-400-500-900-700-701-702-703-1082-10181-62** | | | | |
| **206** | **Bellows ( Bellows )  Part N° S91331Model: 4M6JLT-JBS-E-15-K and JBS-E** | | **ROOM** | **10** |
| **207** | **Bellows ( Bellows )  Part N° S91773 Model: 6R10-JBS-E-35-KConst : TYCO** | | **ROOM** | **10** |
| **208** | **Bellows (Bellows)  Part N° S91335Model: 4P6JLT-JBS-E-15-K and JBS-EConst: TYCO** | | **ROOM** | **10** |
| **209** | **Bellows (Bellows)  Part N° S91325Model: 1,5F2JLT-JBS-E-15-K and JBS-EConst: TYCO** | | **ROOM** | **10** |
| **210** | **Bellows (Bellows)  Part N° S91740Model: 1E2JLT-JBS-E-15-K and JBS-EConst: TYCO** | | **ROOM** | **10** |
| **211** | **Bellows (Bellows)  Part N° S91743Model: 3L4JLT-JBS-E-15-K and JBS-EConst: TYCO** | | **ROOM** | **10** |
| **PDR for PSV valve 9511012E unit: 700-701** | | | | |
| **212** | **Spring Steel  PSV Model: 9511012E** | | **ROOM** | **6** |
| **213** | **Disc Holder  Model: 9511012E** | | **ROOM** | **6** |
| **214** | **O-Ring Kit  Model: 9511012E** | | **ROOM** | **6** |
| **PDR for valve PSV 1E2 JOS-E-35-N2-K unit: 700-701** | | | | |
| **215** | **Disc Holder  PSV Model: 1E2 JOS-E-35-N2-K** | | **ROOM** | **6** |
| **216** | **O-Ring kit  Model: 1E2 JOS-E-35-N2-K** | | **ROOM** | **6** |
| **PDR for PSV valve 9511011E unit: 700-701** | | | | |
| **217** | **Disc Holder  PSV Model: 9511011E** | | **ROOM** | **20** |
| **218** | **O-Ring Kit  Model: 9511011E** | | **ROOM** | **20** |
| **219** | **Spring  PSV Model: 9511011E** | | **ROOM** | **20** |
| **PDR for valve PSV 1D2 JOS-E-35-K unit: 10-700-701** | | | | |
| **220** | **O-Ring Kit  Model: 1D2 JOS-E-35-K** | | **ROOM** | **6** |
| **221** | **Disc Holder  PSV Model: 1D2 JOS-E-35-K** | | **ROOM** | **6** |
| **PDR for valve PSV 1.5F2 JOS-E-35-K unit: 700-701** | | | | |
| **222** | **Spring (KIT)  Model: 1,5F2 JOS-E-35-K** | | **ROOM** | **6** |
| **223** | **Disc Holder  PSV Model: 1.5F2 JOS-E-35-K** | | **ROOM** | **6** |
| **224** | **O-Ring Kit  Model: 1.5F2 JOS-E-35-K** | | **ROOM** | **6** |
| **PDR for valve PSV 4M6 JOS-E-35-M4-K unit: 700-701** | | | | |
| **225** | **Spring (KIT)  Model: 4M6 JOS-E-35-M4-K** | | **ROOM** | **6** |
| **226** | **Disc Holder  Model: 4M6 JOS-E-35-M4-K** | | **ROOM** | **6** |
| **227** | **O-Ring Kit  Model: 4M6 JOS-E-35-M4-K** | | **ROOM** | **6** |
| **PDR for valve PSV 3J4 JOS-E-35-M4-K unit: 700-701** | | | | |
| **228** | **Spring (KIT)  PSV Model: 3J4 JOS-E-35-M4-K** | | **ROOM** | **6** |
| **229** | **Disc Holder  PSV Model: 3J4 JOS-E-35-M4-K** | | **ROOM** | **6** |
| **230** | **O-Ring Kit  Model: 3J4 JOS-E-35-M4-K** | | **ROOM** | **6** |
| **PDR for unit: 100-11-1082-10 PSV 3K4 JBS-E-15-E** | | | | |
| **231** | **O-Ring Kit  Model: 3K4 JBS-E-15-E** | | **ROOM** | **6** |
| **PDR for unit: 100-11-1082-10 PSV 1.5G3 JBS-E-15-K** | | | | |
| **232** | **Spring (KIT)  Model: 1.5G3 JBS-E-15-K Part No: SX36081-102713** | | **ROOM** | **6** |
| **233** | **Disc Holder  Model: 1.5G3 JBS-E-15-K Part No: 147156** | | **ROOM** | **6** |
| **234** | **O-Ring Kit  Model: 1.5G3 JBS-E-15-K** | | **ROOM** | **6** |
| **PDR for unit: 63/1070/1031/1082/1081 PSV 9511111B** | | | | |
| **237** | **Spring  Model: 9511111B** | | **ROOM** | **3** |
| **238** | **Disc Holder  Model: 9511111B** | | **ROOM** | **3** |
| **239** | **O-Ring kit  Model: 9511111B** | | **ROOM** | **3** |
| **PDR for valve PSV 2H3 JOS-E-35-K unit: 700-701** | | | | |
| **240** | **Spring  PSV Model: 2H3 JOS-E-35-K** | | **ROOM** | **6** |
| **241** | **Disc Holder  PSV Model: 2H3 JOS-E-35-K** | | **ROOM** | **6** |
| **242** | **O-Ring Kit  Model: 2H3 JOS-E-35-K** | | **ROOM** | **6** |
| **PDR for unit: 100-11-1082-10 PSV 46305-810/S1** | | | | |
| **243** | **Piston Seal  PSV Model: 46305-810/S1** | | **ROOM** | **6** |
| **244** | **Seat  Model: 46305-810/S1** | | **ROOM** | **6** |
| **245** | **Linear Seal  PSV Model: 46305-810/S1** | | **ROOM** | **6** |
| **246** | **Spring  Model: 46305-810/S1** | | **ROOM** | **6** |
| **247** | **Disc Holder  Model: 46305-810/S1** | | **ROOM** | **6** |
| **248** | **O-Ring Kit  Model: 46305-810/S1** | | **ROOM** | **6** |
| **PDR for unit: 100-200-1080-1051-600-63-1031-11 PSV 9511011E** | | | | |
| **249** | **Seat  Model: 9511011E** | | **ROOM** | **20** |
| **250** | **Piston Seal  Model: 9511011E** | | **ROOM** | **20** |
| **251** | **Linear Seal  Model: 9511011E** | | **ROOM** | **20** |
| **PDR for unit: 100-1080-1051-600-63-1031-11 PSV 9511011B** | | | | |
| **252** | **Seat  Model: 9511011B** | | **ROOM** | **50** |
| **253** | **Piston Seal  Model: 9511011B** | | **ROOM** | **50** |
| **254** | **Linear Seal  Model: 9511011B** | | **ROOM** | **50** |
| **255** | **Spring  Model: 9511011B Part No: X09745** | | **ROOM** | **50** |
| **256** | **Disc Holder  Model: 9511011B Part No: 121392** | | **ROOM** | **50** |
| **257** | **O-Ring Kit  Model: 9511011B** | | **ROOM** | **50** |
| **PDR for unit: 100-11-1082-10 PSV 6Q8 JBS-E15-K** | | | | |
| **258** | **Spring  Model: 6Q8 JBS-E15-SPL TYPE K** | | **ROOM** | **6** |
| **259** | **Disc Holder  Model: 6Q8 JBS-E15-SPL TYPE K** | | **ROOM** | **6** |
| **260** | **O-Ring Kit  Model: 6Q8 JBS-E15-SPL TYPE K** | | **ROOM** | **6** |
| **PDR for unit: 702-PSV-1601A** | | | | |
| **261** | **Disc Holder: 316L SST  N°5 on drawingModel: 3K4 JOS-E-37-S SPL TYPE E** | | **ROOM** | **1** |
| **262** | **Disc Insert  N°8 on drawing: ASME SA479 TYPE 316 Model: 3K4 JOS-E-37-S SPL TYPE E** | | **ROOM** | **1** |
| **263** | **Gasket (Guide)  N°28 on drawing Soft annealed 316 SSTModel: 3K4 JOS-E-37-S SPL TYPE E** | | **ROOM** | **1** |
| **264** | **Spring: Inconel X-750  N°18 on drawing Model: 3K4 JOS-E-37-S SPL TYPE E** | | **ROOM** | **1** |
| **265** | **Nozzle: ASME SA351 GR-CF8M  N°2 on drawing Model: 3K4 JOS-E-37-S SPL TYPE E** | | **ROOM** | **1** |
| **PDR for unit: 200-PSV-1503** | | | | |
| **266** | **Spring: Chrome Steel  For PSV: Inlet 1" 150RF Outlet: 2" 150RFModel: 1D2 JBS-E-15-SPL TYPE K** | | **ROOM** | **2** |
| **267** | **Nozzle: ASME SA351 GR-CF8M  For PSV: Inlet 1" 150RF Outlet: 2" 150RFModel: 1D2 JBS-E-15-SPL TYPE K** | | **ROOM** | **2** |
| **268** | **Disc Holder: SST361L  For PSV: Inlet 1" 150RF Outlet: 2" 150RFModel: 1D2 JBS-E-15-SPL TYPE K** | | **ROOM** | **2** |
| **PDR for unit: 200-PSV-2501 A/B** | | | | |
| **269** | **Bellows: Incnel 625  For PSV: Inlet 4" 150RF Outlet: 6" 150RFModel: 4M6 JBS-E-15-K** | | **ROOM** | **2** |
| **270** | **Nozzle: ASME SA351 GR-CF8M  For PSV: Inlet 4" 150RF Outlet: 6" 150RFModel: 4M6 JBS-E-15-K** | | **ROOM** | **2** |
| **PDR for unit: 500-PSV-1801A/B** | | | | |
| **271** | **Bellows: Incnel 625  For PSV: Inlet 4" 150RF Outlet: 6" 150RFModel: 4N6 JBS-E-15-K** | | **ROOM** | **2** |
| **272** | **Nozzle  For PSV: Inlet 4" 150RF Outlet: 6" 150RFModel: 4N6 JBS-E-15-K** | | **ROOM** | **2** |
| **PDR for unit: 200-PSV-1702 A/B** | | | | |
| **273** | **Spring (KIT)  For PSV: Inlet 3" 150RF Outlet: 4" 150RFModel: 3K4 JBS-E-15-K** | | **ROOM** | **2** |
| **274** | **Nozzle: SST SA351-CF8M  For PSV: Inlet 3" 150RF Outlet: 4" 150RFModel: 3K4 JBS-E-15-K** | | **ROOM** | **2** |
| **PDR for unit: 200-PSV-1801A/B** | | | | |
| **275** | **Spring (KIT)  For PSV: Inlet 3" 150RF Outlet: 4" 150RFModel: 3L4 JBS-E-15-K** | | **ROOM** | **2** |
| **276** | **Nozzle: SST SA351-CF8M  For PSV: Inlet 8" 300RF Outlet: 10" 300RFModel: 3L4 JBS-E-15-K** | | **ROOM** | **2** |
| **PDR for unit: 200-PSV-2301A/B** | | | | |
| **277** | **Nozzle: SST SA351-CF3M  For PSV: Inlet 8" 300RF Outlet: 10" 300RFModel: 8T10 JBS-E-15-K** | | **ROOM** | **2** |
| **278** | **Spring (KIT)  For PSV: Inlet 8" 300RF Outlet: 10" 300RFModel: 8T10 JBS-E-15-K** | | **ROOM** | **2** |
| **PDR for unit: 200-PSV-2102A/B** | | | | |
| **279** | **Spring (KIT)  For PSV: Inlet 6" 150RF Outlet: 8" 150RFModel: 6R8 JBS-E-15-K** | | **ROOM** | **2** |
| **280** | **Disc Insert  For PSV: Inlet 6" 150RF Outlet: 8" 150RFModel: 6R8 JBS-E-15-K** | | **ROOM** | **2** |
| **281** | **Disc Holder  For PSV: Inlet 6" 150RF Outlet: 8" 150RFModel: 6R8 JBS-E-15-K** | | **ROOM** | **2** |
| **PDR for unit: 200-PSV-2005** | | | | |
| **282** | **Spring  For PSV: Inlet 3/4" 150RF Outlet: 1" 150RFModel: 9511812E Part N°: X09369** | | **ROOM** | **1** |
| **283** | **Disc Insert  For PSV: Inlet 3/4" 150RF Outlet: 1" 150RFModel: 9511812E Part N°: 121391** | | **ROOM** | **1** |
| **284** | **Disc Holder  For PSV: Inlet 3/4" 150RF Outlet: 1" 150RFModel: 9511812E Part N°: 125278** | | **ROOM** | **1** |
| **PDR for unit: 200-PSV-2004 A/B** | | | | |
| **285** | **Spring  For PSV: Inlet 3/4" 150RF Outlet: 1" 150RFModel: BP513812B** | | **ROOM** | **3** |
| **286** | **Disc Insert  For PSV: Inlet 3/4" 150RF Outlet: 1" 150RFModel: BP513812B** | | **ROOM** | **3** |
| **PDR for unit: 200-PSV-2901** | | | | |
| **287** | **Spindle: SST A479-316  For PSV: Inlet 3/4" 150RF Outlet: 1" 150RFModel: 81PS1S6A8A-4** | | **ROOM** | **1** |
| **288** | **Seat: See soft goods  For PSV: Inlet 3/4" 150RF Outlet: 1" 150RFModel: 81PS1S6A8A-4** | | **ROOM** | **1** |
| **289** | **Spring: SST SA479-316  For PSV: Inlet 3/4" 150RF Outlet: 1" 150RFModel: 81PS1S6A8A-4** | | **ROOM** | **1** |
| **PDR for unit: 200-PSV-2004 A/B** | | | | |
| **290** | **Disc Holder  For PSV: Inlet 3/4" 150RF Outlet: 1" 150RFModel: BP513812B** | | **ROOM** | **3** |
| **PDR for PSV valve model 45312D12/SA unit 1081-700-701-703-100** | | | | |
| **291** | **Seat liner  Model PSV 45312D12/SAN° 06 On Drawing** | | **ROOM** | **8** |
| **PDR for PSV valve model 44310H153/S1 unit 1081-700-701-100** | | | | |
| **292** | **Piston seal  Model PSV 44310H153/S1N° 13 On Drawing** | | **ROOM** | **8** |
| **293** | **Seat  Model PSV 44310H153/S1N° 7 On Drawing** | | **ROOM** | **8** |
| **294** | **Linear seal  Model PSV 44310H153/S1N° 06 On Drawing** | | **ROOM** | **8** |
| **PDR for PSV valve model 1.5F2 JLT-JOS-E-15-E unit 10-1070-1051-701** | | | | |
| **295** | **Disc holder  Model PSV 1.5F2 JLT-JOS-E-15-E** | | **ROOM** | **6** |
| **PDR for PSV valve for unit 10-11-100-30-31-200-1120-1121-1060-1070-400-500-900-700-701-702-703-1082-1081-62** | | | | |
| **296** | **Bellows (Bellows) (EX:10-PSV-1858A/S ,SN:11-04900/04901)  Model: 3K4JLT-JBS-E-15-K Part N° S91742** | | **ROOM** | **10** |
| **297** | **Bellows (Bellows) (702-PSV-2001A ,SN:11-07509)  Model: 4N6JLT-JBS-E-15-N2-K and JBS-E Part N° S91332** | | **ROOM** | **10** |
| **PDR for unit: 200-PSV-2003A-2003B-2003C-2902-1103** | | | | |
| **298** | **Spring SST 316  For PSV: Inlet 3/4" 300RF Outlet: 1" 150RFModel: 81PS1S6B8A-4** | | **ROOM** | **6** |
| **299** | **Disc insert AST4140/ZN CO  For PSV: Inlet 3/4" 300RF Outlet: 1" 150RFModel: 81PS1S6B8A-4** | | **ROOM** | **6** |
| **300** | **Spindle SST A479-316  For PSV: Inlet 3/4" 300RF Outlet: 1" 150RFModel: 81PS1S6B8A-4** | | **ROOM** | **6** |
| **PDR for unit: 700-701-11-1051-1071-1061-1031-1081-31-1082-1060-100** | | | | |
| **301** | **Disc insert (Ex:100-PSV- 2204, SN:11-05722)  Model: 1.5F2 JBS-E-15-SPL TYPE KPart No: 136978** | | **ROOM** | **10** |
| **302** | **Disc insert (EX:1051-PSV-1204A/ D , SN:11-07648/49)  Model: 8T10JOS-HE-35-CPart No: 145874** | | **ROOM** | **10** |
| **303** | **Spring (KIT) (EX:10-PSV-60A , SN:11-28857)  Model: 6Q8 JBS-E16-K Part No:SX07808** | | **ROOM** | **10** |
| **304** | **Spring (KIT) (EX:10-PSV-38A/S , SN:11-04915/16)  Model: 8T10 JBS-E45-K Part No: SX36056** | | **ROOM** | **10** |
| **PDR for PSV valve 9511012B-SPL unit 701-703-1091** | | | | |
| **305** | **Spring  Model: 9511012B-SPL** | | **ROOM** | **6** |
| **306** | **Disc holder  Model: 9511012B-SPL** | | **ROOM** | **6** |
| **307** | **O-Ring Kit  Model: 9511012B-SPL** | | **ROOM** | **6** |
| **PDR for valve PSV 1.5F2 JBS-E16-SPL TYPE K unit 701-703-1091** | | | | |
| **308** | **Tailpiece  Model: 1.5F2 JBS-E16-K** | | **ROOM** | **6** |
| **309** | **Disc insert  Model: 1.5F2 JBS-E16-K** | | **ROOM** | **6** |
| **310** | **Bellows  Model: 1.5F2 JBS-E16-M** | | **ROOM** | **6** |
| **311** | **Disc holder  Model: 1.5F2 JBS-E16-K** | | **ROOM** | **6** |
| **PDR for valve PSV 1.5 G3 JBS-E-25-K unit 701-703-1091** | | | | |
| **312** | **Disc holder  Model: 1.5G3 JBS-E-25-K** | | **ROOM** | **6** |
| **PDR for valve PSV 6R10 JBS-E-35-K unit 31-11-10-700** | | | | |
| **313** | **Disc holder  Model: 6R10 JBS-E-35-K** | | **ROOM** | **6** |
| **PDR for valve PSV 4M6 JBS-E-15-N2-K unit 31-11-10-700** | | | | |
| **314** | **Disc holder  Model: 4M6 JBS-E-15-N2-K** | | **ROOM** | **6** |
| **PDR for PSV valve 4L6-JOS-HE-37-SPL TYPE C unit 31-11-10-700** | | | | |
| **315** | **Disc holder  Model: 4L6-JOS-HE-37-SPL TYPE C** | | **ROOM** | **6** |
| **PDR for PSV valve 3L4-JLT-JBS-E-15-K unit 31-11-10-700** | | | | |
| **316** | **Disc holder  Model: 3L4-JLT-JBS-E-15-K** | | **ROOM** | **6** |
| **PDR for valve PSV 1.5F2 JLT-JOS-E-35-K unit 31-11-10-700** | | | | |
| **317** | **Disc holder  Model: 1.5F2 JLT-JOS-E-35-K** | | **ROOM** | **6** |
| **PDR for valve PSV 6R10 JLT-JBS-E-45-K unit 31-11-10-700** | | | | |
| **318** | **Bushing  PSV Model: 6R10 JLT-JBS-E-45-SPL TYPE K** | | **ROOM** | **6** |
| **319** | **Disc holder  PSV Model: 6R10 JLT-JBS-E-45-SPL TYPE K** | | **ROOM** | **6** |
| **PDR for PSV valve 4P6-JBS-E-15-K unit 31-11-10-700** | | | | |
| **320** | **Disc holder  PSV Model: PSV 4P6-JBS-E-15-K** | | **ROOM** | **6** |
| **PDR for valve 1E2 JLT-JBS-E-15-K unit 30-31-11-10-700** | | | | |
| **321** | **Disc holder  PSV Model: 1E2 JLT-JBS-E-15-K** | | **ROOM** | **6** |
| **PDR for valve PSV 1.5G3 JBS-E-15-K** | | | | |
| **322** | **Disc holder  PSV Model: 1.5G3 JBS-E-15-K** | | **ROOM** | **6** |
| **PDR for valve PSV 8T10 JBS-E-15-N2-K unit 1081-700-701-702-100** | | | | |
| **323** | **Disc insert  PSV Model: 8T10 JBS-E-15-N2-K** | | **ROOM** | **6** |
| **324** | **Disc holder  PSV Model: 8T10 JBS-E-15-N2-K** | | **ROOM** | **6** |
| **PDR for PSV valve 8T10 JLT-JBS-E-15--K unit 1081-700-701-100** | | | | |
| **325** | **Disc holder  PSV Model: 8T10 JLT-JBS-E-15--K** | | **ROOM** | **6** |
| **PDR for valve PSV 1D2 JOS-E-35-E unit 1081-700-701-703-100** | | | | |
| **326** | **Disc holder  PSV Model: 1D2 JOS-E-35-E** | | **ROOM** | **6** |
| **PDR for PSV valve 45312D12/S1unit 1081-700-701-100** | | | | |
| **327** | **Piston Seat  PSV Model: 45312D12/S1 N° 13 On drawing** | | **ROOM** | **8** |
| **For 400-PSV-1903A-1903B/2003A/2003B/2103A/2103B 400-PSV-2203A-2203B/2203A/2303B/2403A/2403B** | | | | |
| **328** | **Disc Holder  PSV model: 3K4 JBS-E22-KS/N: 11-06811-11-06812Inlet: 3'' 300 RFOutlet: 4'' 150 RF Set Pressure: 10.5KG/CM2G** | | **ROOM** | **3** |
| **400-PSV-3602A/3602B; 400-PSV-1103/1104** | | | | |
| **329** | **Disc Insert  PSV Model: 1D2 JLT-JBS-E-35-KS/N: 11-06775Inlet: 1/2'' 300 RFOutlet: 2'' 150 RF Set Pressure: 27KG/CM2G** | |  | **2** |
| **330** | **Spring  PSV MODEL: 1D2 JLT-JBS-E-35-KS/N: 11-06775INLET: 1/2'' 300RFOUTLET:2'' 150RFSET PRESSURE: 27KG/CM2G** | |  | **2** |
| **331** | **DISC HOLDER  PSV MODEL: 1D2 JLT-JBS-E-35-KS/N: 11-06775Inlet: 1/2'' 300 RFOutlet: 2'' 150 RF Set Pressure: 27KG/CM2G** | |  | **2** |
| **332** | **Spindle  PSV Model: 1D2 JLT-JBS-E-35-KS/N: 11-06775Inlet: 1/2'' 300RFSet Pressure: 27KG/CM2G** | |  | **2** |
| **333** | **Disc Insert  PSV Model: 1D2 JLT-JBS-EK S/N: 11-06778INLET: 1/2'' 300RFOUTLET: 2'' 150RFSET PRESSURE: 11.8KG/CM2G** | |  | **3** |
| **334** | **Spring  PSV MODEL: 1D2 JLT-JBS-E-15-KS/N: 11-06778INLET: 1/2'' 300RFOUTLET:2'' 150RFSET PRESSURE: 11.8KG/CM2G** | |  | **3** |
| **335** | **Disc Holder  1D2 JLT-JBS-E-15-KS/N: 11-06778INLET: 1/2'' 300RFOUTLET: 2'' 150RFSET PRESSURE: 11.8KG/MG** | |  | **3** |
| **336** | **Spindle  1D2 JLT-JBS-E-15-KS/N: 11-06778INLET: 1/2'' 300RFOUTLET: 2'' 150RFSET PRESSURE: 11.8KG/CM2G** | |  | **3** |
| **400-PSV-1110** | | | | |
| **337** | **Disc Insert  PSV MODEL: 1.5F2 JLT-JBS-E-36-KS/N: 11-06920Inlet: 1/5'' 300 RFOutlet: 2'' 150 RF Set Pressure: 27KG/CM2G** | |  | **1** |
| **338** | **SPRING  PSV MODEL: 1.5F2 JLT-JBS-E-36-KS/N: 11-06920Inlet: 1/5'' 300 RFOutlet: 2'' 150 RF Set Pressure: 27KG/CM2G** | |  | **1** |
| **339** | **DISC HOLDER  PSV MODEL: 1.5F2 JLT-JBS-E-36-KS/N: 11-06920Inlet: 1/5'' 300RFOutlet: 2'' 150RFSet Pressure: 27KG/CM2G** | |  | **1** |
| **340** | **Spindle  PSV MODEL: 1.5F2 JLT-JBS-E-36-KS/N: 11-06920Inlet: 1/5'' 300RFOutlet: 2'' 150RFSet Pressure: 27KG/CM2G** | |  | **1** |
| **400-PSV-1202A/1202B 400-PSV-1203A** | | | | |
| **341** | **Disc Insert  PSV MODEL: 3L4 J-JBS-E-26-KS/N: 11-06920Inlet: 1/5'' 300RFOutlet: 2'' 150RFSet Pressure: 3.5KG/CM2G** | |  | **2** |
| **342** | **Spring  PSV MODEL: 3L4 J-JBS-E-26-KS/N: 11-06920Inlet: 1/5'' 300RFOutlet: 2'' 150RFSet Pressure: 3.5KG/CM2G** | |  | **2** |
| **343** | **Disc Holder  PSV Model: 3L4 JBS-E-26-KS/N: 11-60477INLET: 3'' 300RFOUTLET: 4'' 150RF Set Pressure: 3.5KG/CM2G** | |  | **2** |
| **344** | **Spindle  PSV Model: 3L4 JBS-E-26-KS/N: 11-60477INLET: 3'' 300RFOUTLET: 4'' 150RFSet Pressure: 3.5KG/CM2G** | |  | **2** |
| **345** | **Spring  PSV Model: 1.5 F2 JBS--E-15-KS/N: 11-06856-11-06857INLET: 1/5'' 300RFOUTLET: 2'' 150RFSet Pressure: 3.5KG/CM2G** | |  | **3** |
| **400-PSV-2002A-2002B** | | | | |
| **346** | **Disc Insert  PSV Model: 1.5G3 JBS-E32-K-SPLS/N:11-06805-11-06816Inlet: 1.5'' 300 RFOutlet: 3'' 150 RF Set Pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **347** | **Spring  PSV model: 1.5G3 JBS-E32-K-SPLS/N:11-06805-11-0680Inlet: 1.5'' 300 RFOutlet: 3'' 150 RF Set Pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **348** | **Disc Holder  PSV model: 1.5G3 JBS-E32-K-SPL S/N: 11-06815-11-06816Inlet: 1.5'' 300RFOutlet: 3'' 150RF Set Pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **FOR-400-PSV-2102A/2102B/2202A/2202B/2302A/2302B/2402A/2402B** | | | | |
| **349** | **Disc Insert  PSV MODEL: 1.5G3 JSB-E22-KInlet: 1.5'' 300RFOutlet: 3'' 150RF SET PRESSURE: 10.5KG/CM2G** | | **ROOM** | **3** |
| **350** | **Spring  PSV Model: 1.5G3 JBS-E22-KInlet: 1.5'' 300RFOutlet: 3'' 150RF Set Pressure:10.5KG/CM2G** | | **ROOM** | **3** |
| **351** | **Disc Holder  PSV Model: 1.5G3 JBS-E22-K S/N: 11-06821-11-06822Inlet: 1.5'' 300RFOutlet: 3'' 150RF Set Pressure: 10.5KG/CM2G** | | **ROOM** | **3** |
| **352** | **Bellows  PSV Model: 1.5G3 JBS-E22-KS/N: 11-06821-11-06822Inlet: 1.5'' 300RFOutlet: 3'' 150RF Set Pressure: 10.5KG/CM2G** | | **ROOM** | **3** |
| **353** | **Gasket Kit  PSV Model: 1.5G3 JBS-E32-KS/N:11-06821-11-06822Inlet: 1.5'' 300 RFOutlet: 3'' 150 RF Set Pressure: 10.5KG/CM2G** | | **ROOM** | **3** |
| **FOR-400-PSV-3501A/3501B/3601A/3601B 200-PSV-1702A-1702B** | | | | |
| **354** | **Spring  PSV Model: 3K4 JBS-E15-KS/N: 11-06879-11-06880Inlet: 3'' 150RFOutlet: 4'' 150RF Set Pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **355** | **Disc Holder  PSV Model: 3K4 JBS-E15-KS/N: 11-06879-11-06880Inlet: 3'' 150RFOutlet: 4'' 150RF Set Pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **FOR-400-PSV-4301A/4301B/4401A/4401B 200-PSV-15031/1504** | | | | |
| **356** | **Disc Insert  PSV Model: 1D2 JBS-E-15-KS/N: 11-06894-11-06895Inlet: 1'' 150RFOutlet: 2'' 150RFSet Pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **357** | **Spring  PSV Model: 1D2 JBS-E-15-KS/N: 11-06894-11-06895Inlet: 1'' 150RFOutlet: 2'' 150RFSet Pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **358** | **Disc Holder  PSV Model: 1D2 JBS-E-15-KS/N: 11-06894-11-06895Inlet: 1'' 150RFOutlet: 2'' 150RFSet Pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **359** | **Bellows  PSV Model: 1D2 JBS-E-15-KS/N: 11-06894-11-06895Inlet: 1.5'' 15RFOutlet: 2'' 150RF Set Pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **FOR-400-PSV-2910/3310** | | | | |
| **360** | **Spring  Model: 9511011E-STM S/N: 11-06859Inlet: 0.75'' 150RFOutlet: 1'' 150RFSet Pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **361** | **Spring  PSV Model: 9511011-STM S/N: 11-06859Inlet: 0.75'' 150 RFOutlet: 1'' 150 RF Set Pressure: 35KG/CM2G** | | **ROOM** | **2** |
| **362** | **Disc Holder  PSV Model: 9511011E-STM S/N: 11-06859 Inlet: 0.75'' 150RFOutlet: 1'' 150RFSet Pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **FOR-400-PSV-5118/5218** | | | | |
| **363** | **Disc Insert  PSV Model: 3J4 JBS-E-35-SK S/N: 11-06906Inlet: 3'' 300RFOutlet: 4'' 150RFSet Pressure: 31KG/CM2G** | | **ROOM** | **2** |
| **364** | **Spring  PSV Model: 3J4 JBS-E-35-SK S/N: 11-06906Inlet: 3'' 300RFOutlet: 4'' 150RFSet Pressure: 31KG/CM2** | | **ROOM** | **2** |
| **365** | **Gasket Kit  PSV Model: 3J4 JBS-E-35-SK S/N: 11-06906Inlet: 3'' 300RFOutlet: 4'' 150RFSet Pressure: 31KG/CM2** | | **ROOM** | **2** |
| **FOR-400-PSV-5103/5123/5131/5134/5142/5145** | | | | |
| **366** | **Disc Holder  PSV Model: 1D2 JBS-E-32-KS/N: 11-06901Inlet: 1'' 300RFOutlet: 2'' 150RFSet Pressure: 31KG/CM2G** | | **ROOM** | **2** |
| **367** | **Spindle  PSV Model: 1D2 JLT-JBS-E-32-KS/N: 11-06901Inlet: 1'' 300RFOutlet: 2''150RFSet Pressure: 31KG/CM2G** | | **ROOM** | **2** |
| **FOR-400-PSV-5203** | | | | |
| **368** | **Bellows  PSV Model: 1.5F2 JBS-E-35-SK S/N: 11-06906Inlet: 1.5'' 300RFOutlet: 2'' 150RF Set Pressure: 20KG/CM2G** | | **ROOM** | **1** |
| **369** | **Disc Holder  PSV Model: 1.5F2 JBS-E-35-S-KS/N: 11-06909Inlet: 1/5'' 300RFOutlet: 2'' 150RFSet Pressure: 20KG/CM2G** | | **ROOM** | **1** |
| **FOR 400-PSV-3602A/3602B** | | | | |
| **370** | **Disc Insert  PSV Model: 1.5G3 JBS-E-25-S-KS/N: 11-06881Inlet: 1.5'' 300RFOutlet: 3''150 RFSet Pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **371** | **Spring  PSV Model: 1.5G3 JBS-E-25-S-KS/N: 11-06881Inlet: 1.5'' 300RFOutlet: 3''150RFSet Pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **372** | **Gasket Kit  PSV Model: 1.5G3 JBS-E-25-S-KS/N: 11-06881Outlet:3''150RFSet Pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **373** | **Bellows Taipiece  PSV Model: 1.5G3 JBS-E-25-SK S/N: 11-06881Inlet: 1.5'' 300RFOutlet: 3'' 150RF Set Pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **374** | **Disc Holder  PSV Model 1.5G3 JBS-E-25-S-KS/N: 11-06881Inlet: 1.5'' 300RFOutlet: 3'' 150RFSet Pressure 10.5KG/CM2G** | | **ROOM** | **2** |
| **FOR 400-PSV-5223/5231/5234** | | | | |
| **375** | **Disc Holder  PSV Model: 1D2 JBS-E-35-S-KS/N: 11-06911Inlet: 1'' 300RFOutlet: 2'' 150RFSet Pressure: 20KG/CM2G** | | **ROOM** | **2** |
| **376** | **Spring  PSV Model: 1D2 JBS-E-15-KS/N: 11-06911Inlet: 1'' 300RFOutlet: 2'' 150RFSet Pressure: 20KG/CM2G** | | **ROOM** | **2** |
| **FOR 400-PSV-5240** | | | | |
| **377** | **Bellows Taipece  PSV Model: 1E2 JBS-E-35-SK S/N: 11-06908Inlet: 1'' 300RFOutlet: 2'' 150RFSet Pressure: 23.4KG/CM2G** | | **ROOM** | **1** |
| **378** | **Disc Holder  PSV Model: 1E2 JBS-E35-S-KS/N: 11-06908Inlet: 1'' 300RFOutlet: 2'' 150 RF Set Pressure: 23.4KG/CM2G** | | **ROOM** | **1** |
| **379** | **Spring  PSV Model: 1E2 JBS-E-35-S-KS/N: 11-06908Inlet: 1'' 300 RFOutlet: 2'' 150 RF Set Pressure: 23.4KG/CM2G** | | **ROOM** | **1** |
| **FOR-400-PSV-5214** | | | | |
| **380** | **Disc Holder  PSV Model: 2H3 JBS-E-35-S-KS/N: 11-06913Inlet: 2'' 300RFOutlet: 3'' 150RFSet Pressure: 20KG/CM2G** | | **ROOM** | **1** |
| **381** | **Spring  PSV Model 2H3 JBS-E-35-S-KS/N: 11-06913Inlet: 2'' 300RFOutlet: 3'' 150RFSet Pressure: 20KG/CM2G** | | **ROOM** | **1** |
| **FOR-400-PSV-4122** | | | | |
| **382** | **Disc Holder  PSV Model: 3J4 JBS-E-32-KS/N: 11-06921Inlet: 3'' 300RFOutlet 4''150RFSet Pressure: 31KG/CM2G** | | **ROOM** | **1** |
| **383** | **Spring  PSV Model: 3J4 JBS-E-35-SK S/N: 11-06921Inlet: 3'' 300RFOutlet: 4'' 150RFSet Pressure: 31KG/CM2** | | **ROOM** | **1** |
| **384** | **Gasket Kit  Model: 3J4 JBS-E-32-k S/N: 11-06921Inlet: 3'' 300RFOutlet: 4'150RFSet Pressure: 31KG/CM2G** | | **ROOM** | **1** |
| **FOR-400-PSV-1702A~H** | | | | |
| **385** | **Spindle  PSV Model: 81PS1S6ASA-4/SPLS/N: 11-06797-11-06804Inlet: 0.75'' 150RFOutlet: 1'' 150RFSet Pressure:12.3KG/CM2G** | | **ROOM** | **3** |
| **386** | **Disc Insert  PSV Model: 81PS1S6A8A-4/SPLInlet: 0.75'' 150RFOutlet:1'' 150RF Set Pressure:12.3KG/CM2G** | | **ROOM** | **3** |
| **387** | **Spring  PSV Model: 81PS1S6A8A-4/SPLS/N: 11-06797-11-06804Inlet: 0.75'' 150RFOutlet: 1'' 150RFSet Pressure:12.3KG/CM2G** | | **ROOM** | **3** |
| **388** | **Spindle  PSV Model:81PSS6A8A-4/SPLS/N: 11-06922-11-06929Inlet: 0.75'' 150RFOutlet: 1'' 150RFSet Pressure: 9.5KG/CM2G** | | **ROOM** | **3** |
| **389** | **Disc Insert  PSV Model: 81PSS6A8A-4/SPLS/N: 11-06922-11-06929Inlet: 0.75'' 150RFOutlet:1'' 150RF Set Pressure:9.5KG/CM2G** | | **ROOM** | **3** |
| **390** | **Spring  PSV Model: 81PS1S6A8A-4/SPLS/N: 11-06922-11-06929Inlet: 0.75'' 150RFOutlet: 1'' 150RFSet Pressure: 9.5KG/CM2G** | | **ROOM** | **3** |
| **FOR-400-PSV-1301A/1301B 400-PSV-1302A/1302B** | | | | |
| **391** | **Disc Insert  PSV Model: 56605-810/S1 S/N: 11-06793-11-067986Inlet: 8'' 150RFOutlet: 10'' 150RF Set Pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **392** | **Spring  PSV Model: 56605-810/S1S/N: 11-06793-11-06796Inlet: 8'' 150RFOutlet: 10'' 150RF Set Pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **393** | **O.Ring Kit  Model: 56605-810/S1S/N: 11-067** | | **Room** | **2** |
| **PDR FOR PSV VALVE MODEL 45312D12/S1 UNIT 1081-700-701-100** | | | | |
| **394** | **Seal  Model PSV 45312D12/S1N°7 on drawingConst: TYCO** | | **ROOM** | **8** |
| **PDR FOR PSV TYCO** | | | | |
| **395** | **Spring  Description: SPR SPRING- FREE LGTH 11.50 ODMAX 5.20 COP/n: X36269 Const: TYCO** | | **ROOM** | **2** |
| **PDR FOR VALVE PSV 3J4 JOS-E-35-E UNIT: 701-703-1091** | | | | |
| **396** | **Disc holder  PSV MODEL No.: 3J4 JOS-E-35-EConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 1E2 JOS-E-25-E UNIT: 701-703-1091** | | | | |
| **397** | **Disc holder  PSV MODEL No.: 1E2 JOS-E-25-EConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 3K4 JLT-JBS-E-15-K UNIT: 31-11-10-700** | | | | |
| **398** | **Disc holder  PSV MODEL No.: 3K4 JLT-JBS-E-15-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 4N6 JBS-15-N2-K UNIT: 31-11-10-700** | | | | |
| **399** | **Disc holder  PSV MODEL No.: 4N6 JBS-15-N2-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 3J4 JOS-E-35-E UNIT: 701-703-1091** | | | | |
| **400** | **Disc holder  PSV MODEL N°: 2J3 JLT-JBS-E-25-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 1,5H3 JBS-E-15-K UNIT: 1081-700-701-100** | | | | |
| **401** | **Disc holder  PSV MODEL No.: 1.5H3 JBS-E-15-K Const: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 3J4 JBS-E-15-K UNIT: 1081-700-701-100** | | | | |
| **402** | **Disc holder  PSV MODEL No.: 3J4 JBS-E-15-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 4M6 JBS-E-15-K UNIT: 701-703-1091** | | | | |
| **403** | **Disc holder  PSV MODEL N°: 4M6 JBS-E-15-KConst: TYCO** | | **ROOM** | **6** |
| **P/Automatic Valve Mod: 2P 05 Type Globe Post Size 3B x 3B CV 125-LIFT 38 MM IPI 3000RF** | | | | |
| **404** | **Positioner  Mod: AO-700 DInpit Singnal 0.2÷1KG/CM2** | | **ROOM** | **2** |
| **PDR Valve PSV JNO 15S1-C UNIT:1051/1061** | | | | |
| **405** | **Disc Holder  PSV Model No.: JNO-15S1-C** | | **ROOM** | **9** |
| **406** | **Spring  Model: 9511012B-SPL** | | **ROOM** | **9** |
| **407** | **Gasket Cap Top  PSV Model No.: JNO-15S1-C** | | **ROOM** | **9** |
| **408** | **Gasket Cap Top  PSV Model No.: JNO-15S1-C** | | **ROOM** | **9** |
| **PDR For PSV Valve No. JLT-JNO-15S1-B UNIT: 1061-1022** | | | | |
| **409** | **Disc Holder  N°06 on DrawingVale PSV N° JLT-JNO-15S-B** | | **ROOM** | **23** |
| **410** | **Spring  N°11 on drawingVale PSV N° JLT-JNO-15S-B** | | **ROOM** | **23** |
| **411** | **Gasket Cap Top  N°30 on drawingPSV Model N°: JLT-JNO-15S1-B** | | **ROOM** | **23** |
| **412** | **Gasket CAP  N°32 On drawingVale PSV N° JLT-JNO-15S-B** | | **ROOM** | **23** |
| **For Vale PSV - Model No. JON-16S1** | | | | |
| **413** | **Disc Holder  N°6 On drawing** | | **ROOM** | **8** |
| **414** | **Spring  N°11 on drawing** | | **ROOM** | **8** |
| **415** | **Disc Holder  N°06 on DrawingVale PSV N° JLT-JNO-15S-B** | | **ROOM** | **8** |
| **416** | **Spring  N°11 on drawingVale PSV N° JLT-JNO-15S-B** | | **ROOM** | **8** |
| **417** | **Gasket Cap Top  N°30 on drawingPSV Model N°: JLT-JNO-15S-B** | | **ROOM** | **8** |
| **418** | **Gasket CAP  N°32 On drawingVale PSV N° JLT-JNO-15S-B** | | **ROOM** | **8** |
| **P/Safety valves** | | | | |
| **419** | **Nozzle P/Valve  Mod JNO-H-47-SSize 4P6-MAT.ASTM A182 GRF 316Serie No. C.95540** | | **ROOM** | **2** |
| **420** | **Nozzle P/Valve  Mod JNO-H-25-S1Size 2J3-MAT.ASTM A182 GRF 316Serie No. C.9379** | | **ROOM** | **2** |
| **421** | **Nozzle For Valve  Mod: JNO/JNB-35-S1-BSize 1 1/2 F2** | | **ROOM** | **1** |
| **422** | **Nozzle For Valve  Mod: JNO/JNB H-35-S1Size 4L6  Mat . A 351 CF 8M/A 182F3-SERIE N°C93025** | | **ROOM** | **18** |
| **423** | **Bellows  Ref. 2H3''Mat.SUS 316C** | | **ROOM** | **2** |
| **424** | **Nozzle P/Valve  Mod.JNB/JNO 35 S1 B/CSize 2H3 MAT.ASTM A 192 GRF 316SERIE C93036** | | **ROOM** | **2** |
| **425** | **Spring P/ Valve  Ref.6073 DIM. 11/2 F.2Type.JNO.35.51.BSet DE TRAGE SRG/CM2** | | **ROOM** | **1** |
| **P/Safety Valve Mod: JNB-35-MH-E S/N C93009-1''300 RFXDX 2'' 150 RF** | | | | |
| **426** | **Valve  Ref: 1D2''Mat: Monel K500** | | **ROOM** | **1** |
| **427** | **Valve  Dim: 1 1/2 2''Mat: ASTM A 182 GRF 316** | | **ROOM** | **2** |
| **428** | **Nozzle  Model: HS 26 S1 Siez: 2J3Mat ASTM A 182 GRF 316 Serial No.: C93026** | | **ROOM** | **1** |
| **429** | **Spring P/Valve  Rep: 6471Dim: 21 1/2 J4Type JND 35.S1B Calibration set: 18 KG/Cm2 Qra-AD** | | **ROOM** | **1** |
| **430** | **Spring P/Valve  Dim 3/4 W1Dim: 21 1/2 J4Type JMB.C.SXB Setting pressure: 18 KG/Cm2 Qra-AD** | | **ROOM** | **1** |
| **431** | **Steel gasket  Rep: 1 1/2'' G 2 1/2''Mat V560 (S10C)** | | **ROOM** | **2** |
| **432** | **Spring P/Valve  Ref: 6205 Dim: 4L6** | | **ROOM** | **1** |
| **P/ Safety valve** | | | | |
| **433** | **Nozzle P/Valve  Mod HS.25.S1 Size 3M6Mat: ASTM A 182 GRF 316Serie N°: C.93021** | | **ROOM** | **2** |
| **434** | **Steel seal  Dim: 2H3Mat V560 (S10L )  Ref: 11/2F'' N°REF: 2H3** | | **ROOM** | **10** |
| **435** | **Nozzle P/Valve  Model: JNO 36 M1 E Size: 4L6Mat: Monel K 500Series n°: C93001** | | **ROOM** | **2** |
| **P/ Safety valve Mat: Monel.K.500 Serial: n°C 93013 QRA/02** | | | | |
| **436** | **Nozzle P/Valve  Mod: JNB 35 M1 E; JNB 36 M1 ESize: 6 Q 8Mat: Monel K 500Series: n° C 93013 QRA/02** | | **ROOM** | **1** |
| **437** | **Nozzle P/Valve  Mod JNO.H 35-SDim: 1'' 1/2 H3Series N°: C 93033Mat: ASTM A 182 GRF 316** | | **ROOM** | **1** |
| **P/ Safety valve Mod: JNB-35-M1-E S/N°:C93013-103-PSV-108** | | | | |
| **438** | **Bellows  Ref. SL-03089-01-3503Mat.SUS 316L** | | **ROOM** | **2** |
| **439** | **Spring P/Valve  Ref: 6211 Dim: 4L6Type JNO 35 S1 BSet of calibration: 16.5kg/cm2** | | **ROOM** | **1** |
| **440** | **Nozzle P/valve  Mod JNO 35 S1 BSize 4L6 Mat,ASTM A 531 CF 8M/A 182F3Serie C93042** | | **ROOM** | **1** |
| **441** | **Nozzle P/ Valve  Mod. JLT.JNB 25.SX.B and 25 S1.B Size 2J3Mat. ASTM A 182 GRF 316  Series No. C 93039** | | **ROOM** | **2** |
| **442** | **Valve  Ref: 4K''Mat: Monel K500** | | **ROOM** | **1** |
| **443** | **Valve  Ref: 2J3 A20-56-02Mat.ASTM A 182 GRF 316** | | **ROOM** | **2** |
| **444** | **Valve  Ref: 4P6Mat: ASTM A 182 GRF 316** | | **ROOM** | **2** |
| **445** | **Spring P/Valve  Ref: 1043 , Type JMB.C.SXB  DIM: 3/4 W1 Setting pressure: 20.9 KG/CM2** | | **ROOM** | **6** |
| **446** | **Spring P/Valve  Ref: 1095Mat: JMB.C.SX.B/ DIM: 3/4 W1Setting pressure: 6KG/CM2** | | **ROOM** | **14** |
| **447** | **Spring P/Valve  Dim 4PC REF 6816Type J.N0 H.47.S1String set: 36KG/CM2** | | **ROOM** | **2** |
| **448** | **Spring For Valve  Ref 6304-DIM: 6Q8Type J.N0 H.25.S1Set of 6KG/CM2** | | **ROOM** | **2** |
| **449** | **Spring P/Valve  Ref 6054-DIM: 2J3Type J.N0 H.25.S1Set of calibration: 6KG/CM2** | | **ROOM** | **2** |
| **450** | **Spring P/Valve  Ref 1107 Type: JMB.C.SXBDim 3/4 W1Taring set 1.4 KG/CM2** | | **ROOM** | **1** |
| **451** | **Spring For Valve  Ref 1402Type JMB.C.SXBDIM 3/4 W1/ SETDE: Taring 13.9KG CM2** | | **ROOM** | **1** |
| **P/ Safety valve** | | | | |
| **452** | **Spring For valve  Ref/6092 DIM 11/2 G.2 1/2Type JNO.35.M1.EStaring set: 43KG/CM2** | | **ROOM** | **2** |
| **453** | **Spring For Valve  Dim: 2J3Ref 7061Type JLT.JNB 25.SX.BTaring set 18.5 KG** | | **ROOM** | **1** |
| **454** | **Spring P/Valve  Ref 6081-DIM 2H3Type JNB 35 S1 BSet of trage 11KG/CM2** | | **ROOM** | **1** |
| **455** | **Spring P/Valve  Ref 6093-DIM 2H3Type JNO 35 S1 BSet of calibration 36KG/CM2** | | **ROOM** | **1** |
| **456** | **Spring For Valve  Dim: 1E2 REF.6014Type JNO H 35 S Calibration set 6KG/CM2** | | **ROOM** | **1** |
| **457** | **Spring For Valve  Type: HS 25-S1Dim: 3 m 6Ref: Q 1159Setting pressure: 36KG/CM2** | | **ROOM** | **1** |
| **458** | **Spring for valve  Ref: 6077Type: JNO H 25-S1Dim: 1'' 1/2 H3Taring set= 6 KG/CM2** | | **ROOM** | **2** |
| **459** | **Nozzel P/Valve  Mod: JMB-C-SXB SiZE 3/4 W1Mat: ASTM.A.182.GRF316SERIE: N°C93007** | | **ROOM** | **20** |
| **460** | **Nozzle P/VALVE  MOD: JNO 35 ME1E JNB 36 M1 ESIZE:2H3 MAT: MONEL.K.500Serie N° C93017** | | **ROOM** | **1** |
| **461** | **Nozzle  MOD: JNO.35.M1.ESIZE 1 E2 MAT: MONEL.K.500SERIE N°C.93005** | | **ROOM** | **2** |
| **462** | **Nozzle P/Valve  MOD: JNO.H.35.S1Mat: ASTM A18GRF316SERIE: C93023** | | **ROOM** | **1** |
| **463** | **Nozzle P/Valve  MOD.JNO-H-25-S1Size 6-Q8 MAT,ASTM A 351 CF 8M/A 182 F3SERIE C93073** | | **ROOM** | **2** |
| **464** | **Valve  Ref: 2J3'' 38425Mat.ASTM A 182 GRF 316** | | **ROOM** | **2** |
| **465** | **Spring P/Valve  Type: H.S26.S1Ref: T 573Dim: 2J3 Pulling pressure 34 kg/cm2** | | **ROOM** | **2** |
| **PDR Valve PSV JNO 15S1-C UNIT:1051/1061** | | | | |
| **466** | **Disc Insert  Model No.: JNO-15S1-C** | | **ROOM** | **9** |
| **467** | **Disc Insert  No. 03 on drawingVale PSV No. JLT-JNO-15S-B** | | **ROOM** | **8** |
| **PDR FOR PSV VALVE N°JLT-JNO-15S1-B UNIT: 1061-1022** | | | | |
| **468** | **Disc Insert  No. 03 on drawingVale PSV No. JLT-JNO-15S1-B** | | **ROOM** | **23** |
| **469** | **Disc Insert  N°03 on drawing** | | **ROOM** | **8** |
| **P/SAFETY VALVE** | | | | |
| **470** | **Nozzle f/valve  Mod: JNB-35-M1-ESize: 3K4 Mat: MONEL K 500Serie N°: C 93015** | | **ROOM** | **2** |
| **PDR for safety valve  type REC 261 Dim: 3" 300 x 4" 150, series 3 x K x 4 103, Fluid: C3H8, pressure: 18Kg/Cm2** | | | | |
| **Serial No. 013328** | | | | |
| **471** | Gasket (seal):  REP: 25MAT: aramid fiber | | PS | 2 |
| **472** | Gasket (seal):  REP: 27MAT: aramid fiber | | PS | 2 |
| **Serial No. 013329 and 013331** | | | | |
| **473** | Spring:  REP: 13 SUP: 9 | | PS | 1 |
| **474** | Disc:  REP: 2 SUS: 304 | | PS | 1 |
| **475** | Nozzle (nose):  REP: 1 SUS: 304 | | PS | 1 |
| **PDR for safety valve  type REC 261, Dim 11/2 "300 x 3" 150, series 1-1/2 x H x 3 103 , Fluid : C3H8, pressure: 18Kg/Cm2** | | | | |
| **Serial No. 013329 and 013331** | | | | |
| **476** | Gasket (seal):  REP: 25Mat: aramid fiber | | PS | 2 |
| **477** | Gasket (seal)  REP: 26 Mat : aramid fiber | | PS | 2 |
| **480** | Gasket (seal):  REP: 27 Mat: aramid fiber | | PS | 2 |
| **481** | Spring (spring):  REP: 26 REF: SUP 9 | | PS | 1 |
| **482** | Disc:  REP: 2 REF: SUS: 304 | | PS | 1 |
| **483** | Nozzle (nose):  REP: 1 REF: SUS: 304 | | PS | 1 |
| **PDR for safety valve  type REC 261, Dim 11/2 "300 x 3" 150, series 2 x J x 3 103, Fluid: C3H8, pressure: 18Kg/Cm2 Serial No. 013330** | | | | |
| **484** | Gasket (seal):  REP: 25MAT: aramid fiber | | PS | 2 |
| **485** | Gasket (seal):  REP: 27MAT: aramid fiber | | PS | 2 |
| **486** | Spring (spring):  REP: 13 REF: SUP 9 | | PS | 1 |
| **487** | Disc (disc):  REP: 2 REF: SUS 304 | | PS | 1 |
| **488** | Nozzle (nose):  REP: 1 REF: SUS 304 | | PS | 1 |
| **PSV MODEL SL431-M** | | | | |
| **489** | SPRING #16 ON DRAWING | | PS | 3 |
| **490** | SPINDLE N° 07 ON DRAWING | | PS | 3 |
| **491** | DISC HOLDER N° 05 ON DRAWING | | PS | 3 |
| **492** | GASKET KIT | | PS | 3 |
| **494** | DISC N° 02 ON DRAWING | | PS | 3 |
| **PSV MODEL SL131** | | | | |
| **494** | SPRING #16 ON DRAWING | | PS | 4 |
| **495** | SPINDLE N° 07 ON DRAWING | | PS | 4 |
| **496** | DISC HOLDER N° 03 ON DRAWING | | PS | 4 |
| **four hundred ninety seven** | GASKET KIT | | PS | 4 |
| **498** | DISC N° 02 ON DRAWING | | PS | 4 |
| **PSV MODEL SL431-M2** | | | | |
| **499** | SPRING #16 ON DRAWING | | PS | 3 |
| **500** | SPINDLE N° 07 ON DRAWING | | PS | 3 |
| **501** | DISC HOLDER N° 05 ON DRAWING | | PS | 3 |
| **502** | GASKET KIT | | PS | 3 |
| **503** | DISC N° 02 ON DRAWING | | PS | 3 |
| **For the substitution of the ( 1051 -PSV-1325)** | | | | |
| **504** | Back Pressure  Valve VSM 11/2'' AISI 150 SET.P.2KG/CM2Brand: Seko | | PS | 1 |
| **PDR for safety valves type model: 1D2 JBS-E-36-SPL TYPE K**  **TAG: 100-PSV-1501A/1501B/1502A Set pressure: 27 KG/CM2 SN° 11-05676**  **DWG: DS 108-4869** | | | | |
| **505** | Disc Insert MTL  ASME SA479 Type 316 PSV Model: 1D2 JBS-E-36-SPL TYPE K  Set pressure: 27 KG/CM2 SN° 11-05676  Item: 08 DWG: DS 108-4869 | | PS | 1 |
| **506** | Disc Holder  MTL: 316L SST PSV Model: 1D2 JBS-E-36-SPL TYPE K  Set pressure: 27 KG/CM2 SN° 11-05676  Item: 05 DWG: DS 108-4869 | | PS | 1 |
| **Valve needed for running reforming unit II (103-PSV-322)** | | | | |
| **507** | A complete TARE A 6 KG/CM2G safety valve with calibration certificate S/N NO: C96457 Requires  a nameplate with the following data :  TAG N°: 103-PSV-322Model: JNO-H-35 S1S/R NO: C96457Dimension: 2'' 300#RF X 3'' 150#RFOrifice: 2 XHX 3Set pressure: 6 KG/CM2GFluid: LP steam | PS | 1 | |
| **Valve needed for running reforming unit II (103-PSV-312)** | | | | |
| **508** | A complete TARE A 6 KG/CM2G safety valve with calibration certificate S/N NO: C93025 Requires  a nameplate with the following data :  TAG N°: 103-PSV-312Model: JNO-H-35 S1S/R NO: C93025Dimension: 4'' 300#RF X 6'' 150#RFOrifice: 4 XLX 6Set pressure: 6 KG/CM2GFluid: LP steam | PS | 1 | |
| **Valve needed for running reforming unit II (103-PSV-311B)** | | | | |
| **509** | A complete TARE A 6 KG/CM2G safety valve with calibration certificate S/N NO: C93024 Requires  a nameplate with the following data :  TAG N°: 103-PSV-311BModel: JNO-H-35 S1S/R NO: C93024Dimension: 1'' 300#RF X 2'' 150#RFOrifice: 1 XEX 2Set pressure: 6 KG/CM2GFluid: LP steam | PS | 1 | |
| **P/ Safety valve** | | | | |
| **510** | Spring P/Valve  Dim: 2H3 REF: 6077Type: JNO. H35-S1  Taring set: 6KG/CM2 | PS | 2 | |
| **511** | Nozzle P/Valve  Dim: 2H3 Mod: JNO. H35-S1  Matt: ASTM A182GRF316 Series No.: C96457 | PS | 1 | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Designation** | | **UM** | **Qty** |
| **PDR FOR UNIT: 500-PSV-1311** | | | | |
| **1** | **Spring  Model No.: BP513012BConst: Tyco** | | **ROOM** | **2** |
| **2** | **Seat  Model No.: BP513012BConst: Tyco** | | **ROOM** | **2** |
| **3** | **Disc  316SST Model No.: BP513012BConst: Tyco** | | **ROOM** | **2** |
| **PDR FOR UNIT: 500-PSV-1201/1202** | | | | |
| **4** | **Spring  N°18 on DrawingModel N°: 1E2 JBS-E-36-SPL-KConst: Tyco** | | **ROOM** | **2** |
| **5** | **Disc Insert  N°8 on DrawingModel N°: 1E2 JBS-E-36-SPL-KConst: Tyco** | | **ROOM** | **2** |
| **6** | **Disc Holder  N°5 on DrawingModel N°: 1E2 JBS-E-36-SPL-KConst: Tyco** | | **ROOM** | **2** |
| **7** | **Nozzle  N°2 on DrawingModel N°: 1E2 JBS-E-36-SPL-KConst: Tyco** | | **ROOM** | **2** |
| **PDR FOR UNIT: 200-PSV-2701/2706** | | | | |
| **8** | **Spring  Inlet 3/4''300RF Outlet: 1''300RFModel No.: 81PS1SB8B-4Const: Tyco** | | **ROOM** | **2** |
| **9** | **Disc Insert  Inlet 3/4''300RF Outlet: 1''300RFModel No.: 81PS1SB8B-4Const: Tyco** | | **ROOM** | **2** |
| **10** | **Spindle  Inlet 3/4''300RF Outlet: 1''300RFModel No.: 81PS1SB8B-4Const: Tyco** | | **ROOM** | **2** |
| **PDR FOR UNIT: 100-1080-1051-600-63-1031-11 PSV 81PS1S6B8A-SERIES 80** | | | | |
| **11** | **Seat  Model No.: 81PS1S6B8A-SERIE 80Const: Tyco** | | **ROOM** | **8** |
| **PDR FOR UNIT: 100-11-1082-10 PSV 44305T810/S1** | | | | |
| **12** | **Piston Seal  Model No.: 44305T810/S1Const: Tyco** | | **ROOM** | **6** |
| **13** | **Seat  Model No.: 44305T810/S1Const: Tyco** | | **ROOM** | **6** |
| **14** | **Linear seal  Model No.: 44305T810/S1Const: Tyco** | | **ROOM** | **6** |
| **15** | **Spring  Model No.: 44305T810/S1Const: Tyco** | | **ROOM** | **6** |
| **16** | **Disc Holder  Model No.: 44305T810/S1Const: Tyco** | | **ROOM** | **6** |
| **PDR FOR UNIT: 100-1080-1051-600-63-1031-11 PSV 81PS1S6B8A-SERIES 80** | | | | |
| **17** | **Spring  Model No.: 81PS1S6B8A-SERIE 80Const: Tyco** | | **ROOM** | **8** |
| **18** | **Spindle seal  Model No.: 81PS1S6B8A-SERIE 80Const: Tyco** | | **ROOM** | **8** |
| **19** | **Stabilizing ring  Model No.: 81PS1S6B8A-SERIE 80Const: Tyco** | | **ROOM** | **8** |
| **20** | **Spindle  Model No.: 81PS1S6B8A-SERIE 80Const: Tyco** | | **ROOM** | **8** |
| **21** | **Guide seal  Model No.: 81PS1S6B8A-SERIE 80Const: Tyco** | | **ROOM** | **8** |
| **22** | **Bushing seal  Model N°: 81PS1S6B8A-SERIE 80Const: Tyco** | | **ROOM** | **8** |
| **PDR FOR UNIT: 100-11-1082-10 PSV 3K4 JBS-E-15E** | | | | |
| **23** | **Bellows  Model No.: 3K4 JBS-E-15EConst: Tyco** | | **ROOM** | **6** |
| **24** | **Spring  Bellows Model No.: 3K4 JBS-E-15EConst: Tyco** | | **ROOM** | **6** |
| **25** | **Disc Holder  Bellows Model No.: 3K4 JBS-E-15EConst: Tyco** | | **ROOM** | **6** |
| **PDR FOR UNIT: 100-11-1082-10 PSV 1.5G3 JBS-E-15-K** | | | | |
| **26** | **Bellows  Model No.: 1.5G3 JBS-E-15-KConst: Tyco** | | **ROOM** | **6** |
| **PDR FOR UNIT: 100-11-1082-10 PSV 8T10 JBS-E-15-K** | | | | |
| **27** | **Disc Holder  Model No.: 8T10 JBS-E-15-KConst: Tyco** | | **ROOM** | **10** |
| **PDR FOR UNIT: 100-11-1082-10 PSV 8T10 JBS-E-45-K** | | | | |
| **28** | **Disc Holder  8T10 JBS-E-45-KConst: Tyco** | | **ROOM** | **6** |
| **PDR FOR PSV 900 SERIES VALVE MODEL 913BGF M06 JEO 145** | | | | |
| **29** | **Cap o-ring  N°23 on Drawing Valve PSV SERIE900 MODEL 913BGF M06 JEO 145Const: KUNKLE (TYCO)** | | **ROOM** | **10** |
| **30** | **Gag screw gasket  N°23 on Drawing PTFEValve PSV SERIE900 MODEL 913BGF M06 JEO 145Const: KUNKLE (TYCO)** | | **ROOM** | **10** |
| **31** | **Spring  Ref: SS A313-316 OR A313-T631/Alloy steel: A681-H12 OR B637-X750Const: KUNKLE (TYCO)** | | **ROOM** | **10** |
| **32** | **O-ring  cap N°12 on Drawing PTFEValve PSV SERIE900 MODEL 913BGF M06 JEO 145Const: KUNKLE (TYCO)** | | **ROOM** | **10** |
| **PDR FOR UNIT: 100-11-1082-10 PSV 6Q8 JBS-E-15-K** | | | | |
| **33** | **Bellows  Model No.: 6Q8 JBS-E-15-KConst: Tyco** | | **ROOM** | **6** |
| **PDR FOR PSV 900 SERIES VALVE MODEL 913BGF M06 JEO 145** | | | | |
| **34** | **O-ring body  N°02 on Drawing PTFEValve PSV SERIE900 MODEL 913BGF M06 JEO 145Const: KUNKLE (TYCO)** | | **ROOM** | **10** |
| **35** | **Disc  Ref: /SS A479-315N°05 on Drawing Valve PSV SERIE900 MODEL 913BGF M06 JEO 145Const: KUNKLE (TYCO)** | | **ROOM** | **10** |
| **36** | **Seal  N°02 on Drawing PTFEValve PSV SERIE900 MODEL 913BGF M06 JEO 145Const: KUNKLE (TYCO)** | | **ROOM** | **10** |
| **37** | **Disc Holder  Ref: BRASS,B16,(SS A351-CF8M Model913,919 ONLYValve PSV SERIE900 MODEL 913BGF M06 JEO 145Const: KUNKLE (TYCO)** | | **ROOM** | **10** |
| **PDR FOR UNIT: 100-1080-1051-600-63-1031-11 PSV 1.5H3 JOS-HE-15-C** | | | | |
| **38** | **Bellows  PSV Model No.: 1.5H3 JOS-HE-15-CConst: Tyco** | | **ROOM** | **6** |
| **39** | **Disc Insert  PSV Model No.: 1.5H3 JOS-HE-15-CConst: Tyco** | | **ROOM** | **6** |
| **40** | **Spring  PSV Model No.: 1.5H3 JOS-HE-15-CConst: Tyco** | | **ROOM** | **6** |
| **41** | **Disc holder  PSV Model No.: 1.5H3 JOS-HE-15-CConst: Tyco** | | **ROOM** | **6** |
| **42** | **o-ring kit  Model No.: 1.5H3 JOS-HE-15-CConst: Tyco** | | **ROOM** | **6** |
| **PDR FOR UNIT: 100-1080-1051-600-63-1031-11 PSV 81PS1S6B8A-SERIES 80** | | | | |
| **43** | **Blowdown adjustment screw seal  Model No.: 81PS1S6B8A-SERIE 80Const: Tyco** | | **ROOM** | **8** |
| **PDR FOR VALVE PSV 1D2 JOS-E35-K UNIT 700-701** | | | | |
| **44** | **Spring  Model No.: 1D2 JOS-E35-KConst: Tyco** | | **ROOM** | **6** |
| **PDR FOR UNIT: 100-11-1082-10 PSV 46305-1014/S1** | | | | |
| **45** | **Spring  PSV Model No.: 46305-1014/S1Const: Tyco** | | **ROOM** | **6** |
| **46** | **Disc holder  PSV Model No.: 46305-1014/S1Const: Tyco** | | **ROOM** | **6** |
| **47** | **Linear seal  PSV Model No.: 46305-1014/S1Const: Tyco** | | **ROOM** | **6** |
| **48** | **Seat  Model No.: 46305-1014/S1Const: Tyco** | | **ROOM** | **6** |
| **49** | **Piston Seal  PSV Model No.: 46305-1014/S1Const: Tyco** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 1E2 JOS-E35-N2-K UNIT 700-701** | | | | |
| **50** | **Spring  Model No.: 1E2 JOS-E35-N2-KConst: Tyco** | | **ROOM** | **6** |
| **PDR FOR UNIT: 100-1080-1051-600-63-1031-11 PSV 6Q8 JBS-E-35-K** | | | | |
| **51** | **O-ring kit  Model No.: 6Q8 JBS-E-35-KConst: Tyco** | | **ROOM** | **6** |
| **52** | **Disc holder  PSV Model No.: 6Q8 JBS-E-35-KConst: Tyco** | | **ROOM** | **6** |
| **53** | **Spring  Model No.: 6Q8 JBS-E-35-KConst: Tyco** | | **ROOM** | **6** |
| **54** | **Bellows  PSV Model No.: 6Q8 JBS-E-35-KConst: Tyco** | | **ROOM** | **6** |
| **PDR FOR UNIT: 700-701-11-1051-1071-1061-1031-1081-31-1082-1060-100** | | | | |
| **55** | **Disc insert  Part N° 145873Model N°: 6R10 JOSH-E & JBS-EConst: Tyco** | | **ROOM** | **10** |
| **PDR FOR UNIT: 900-PSV-1401/1402** | | | | |
| **56** | **Spring for PSV  CRM STL/1215 STLPart No. SX36026-103200Model No.: 1D2 JBS-E-35-KConst: Tyco** | | **ROOM** | **2** |
| **57** | **Disc insert for PSV  SST SAA479-316Part No. 136977Model No.: 1D2 JBS-E-35-KConst: Tyco** | | **ROOM** | **2** |
| **58** | **Disc holder for PSV  SST SAA479-316LPart No. 147151Model No.: 1D2 JBS-E-35-KConst: Tyco** | | **ROOM** | **2** |
| **59** | **Nozzle for PSV  SST SA351-CF8MSST SAA479-316Part No. 103185Model No.: 1D2 JBS-E-35-KConst: Tyco** | | **ROOM** | **2** |
| **PDR FOR UNIT: 500-PSV-5501/900-PSV-1101A/B** | | | | |
| **60** | **Spring for PSV  Inconel X-750Model No: 1E2 JBS-E-16-KConst: Tyco** | | **ROOM** | **3** |
| **61** | **Disc insert for PSV  ASME SA479TYPE 316Model No: 1E2 JBS-E-16-KConst: Tyco** | | **ROOM** | **3** |
| **62** | **Disc holder for PSV  316 L SST Model No.: 1E2 JBS-E-16-KConst: Tyco** | | **ROOM** | **3** |
| **63** | **Nozzle for PSV  ASME SA351 GR CF8M Model No.: 1E2 JBS-E-16-KConst: Tyco** | | **ROOM** | **3** |
| **PDR FOR UNIT: 500-PSV-1901** | | | | |
| **64** | **Spring for PSV  CRM STL/1215 STLPart No. SX36076-102713Model No.: 1.5G3 JIS-HE-15-CConst: Tyco** | | **ROOM** | **2** |
| **65** | **Disc insert for PSV  SST SA479-315Part No. 136979Model No.: 1.5G3 JIS-HE-15-CConst: Tyco** | | **ROOM** | **2** |
| **66** | **Disc holder for PSV  SST SA351-CF3MPart No. 147156Model No.: 1.5G3 JIS-HE-15-CConst: Tyco** | | **ROOM** | **2** |
| **67** | **Nozzle for PSV  SST SA351-CF8MPart No. 102813Model No.: 1.5G3 JIS-HE-15-CConst: Tyco** | | **ROOM** | **2** |
| **PDR FOR UNIT: 500-PSV-1702** | | | | |
| **68** | **Spring for PSV  Model No.: 9511X12E-SPLConst: Tyco** | | **ROOM** | **2** |
| **69** | **Seat for PSV  Model No.: 9511X12E-SPLConst: Tyco** | | **ROOM** | **2** |
| **70** | **Disc for PSV  Model No.: 9511X12E-SPLConst: Tyco** | | **ROOM** | **2** |
| **PDR FOR UNIT: 500-PSV-1603A/B** | | | | |
| **71** | **Spring for PSV  Model No.: 1D2 JBS-E-25X-K-SPL-SPLConst: Tyco** | | **ROOM** | **2** |
| **72** | **Seat for PSV  Model No.: 1D2 JBS-E-25X-K-SPL-SPLConst: Tyco** | | **ROOM** | **2** |
| **73** | **Disc for PSV  Model No.: 1D2 JBS-E-25X-K-SPL-SPLConst: Tyco** | | **ROOM** | **2** |
| **PDR FOR UNIT: 500-PSV-1601A/B** | | | | |
| **74** | **Spring for PSV  No. 18 on drawingModel No.: 8T10 JBS-E-35-KConst: Tyco** | | **ROOM** | **2** |
| **75** | **Disc insert for PSV  N° 08 on drawingModel N°: 8T10 JBS-E-35-KConst: Tyco** | | **ROOM** | **2** |
| **76** | **Disc holder for PSV  No. 05 on drawingModel No.: 8T10 JBS-E-35-KConst: Tyco** | | **ROOM** | **2** |
| **77** | **Nozzle for PSV  N° 02 on drawingModel N°: 8T10 JBS-E-35-KConst: Tyco** | | **ROOM** | **2** |
| **PDR FOR UNIT: 700-701-11-1051-1071-1061-1031-1081-31-1082-1060-100** | | | | |
| **78** | **Spring  Part No. SX36375 Model No.: 8T10 JOS-HE-35-CConst: Tyco** | | **ROOM** | **10** |
| **79** | **Spring  Part No. SX36373 Model No.: 8T10 JBS-E-15-KConst: Tyco** | | **ROOM** | **10** |
| **80** | **Spring  Part No. SX36077 Model No.: 1.5H3 JLT-JBS-E-15-KConst: Tyco** | | **ROOM** | **10** |
| **81** | **Spring  Part No. SX36073 Model No.: 1.5H2 JLT-JBS-E-15-KConst: Tyco** | | **ROOM** | **10** |
| **82** | **Spring  Part No. SX36031 Model No.: 1D JOS-E-35-KConst: Tyco** | | **ROOM** | **10** |
| **83** | **Spring  Part No. SX36308 Model No.: 6Q8 JBS-E-35-KConst: Tyco** | | **ROOM** | **10** |
| **84** | **Spring  Part No. SX36156 Model No.: 3K4 JBS-E-OR-35-KConst: Tyco** | | **ROOM** | **10** |
| **85** | **Spring  Part No. SX36380 Model No.: 8T10 JOS-HE-45-CConst: Tyco** | | **ROOM** | **10** |
| **86** | **Spring  Part No. SX36375 Model No.: 8T10 JOS-HE-35-CConst: Tyco** | | **ROOM** | **10** |
| **87** | **Spring  Part No. SX36374 Model No.: 8T10 JOS-HE-35-CConst: Tyco** | | **ROOM** | **10** |
| **PDR FOR VALVE PSV 4L6 JOS-E35-N2-K UNIT: 700-701** | | | | |
| **88** | **Spring  Model No.: 4L6 JOS-E35-N2-KConst: Tyco** | | **ROOM** | **6** |
| **89** | **Disc holder  Model No.: 4L6 JOS-E35-N2-KConst: Tyco** | | **ROOM** | **6** |
| **90** | **O-ring kit  Model No.: 4L6 JOS-E35-N2-KConst: Tyco** | | **ROOM** | **6** |
| **PDR FOR UNIT: 100-11-1051-1082-10 PSV 46305-1014/S1** | | | | |
| **91** | **O-ring kit  Model No: 46305-1014/S1 Const: Tyco** | | **ROOM** | **6** |
| **PDR FOR PSV VALVE MODEL 26305-810/S1 UNIT 1070-1051-701** | | | | |
| **92** | **Bonnet seat  MODEL PSV 26305-810/S1N°08 on drawingConst: Tyco** | | **ROOM** | **6** |
| **93** | **Seat  MODEL PSV 26305-810/S1N°04 on drawingConst: Tyco** | | **ROOM** | **6** |
| **94** | **Nozzle seat  MODEL PSV 26305-810/S1N°02 on drawingConst: Tyco** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV MODEL 8T210 JOS-HE-15-C-SPL UNIT 1070-1051-701** | | | | |
| **95** | **Disc holder  MODEL PSV 8T210 JOS-HE-15-C-SPLConst: Tyco** | | **ROOM** | **6** |
| **FOR 400-PSV-1903A-1903B/2003A/2003B/2103A/2103B/400-PSV-2203A-2203B/2303A/2303B/2403A/2403B** | | | | |
| **96** | **Spring  MODEL PSV 3K4 JBS-E22-KS/N: 11-06811-06812Inlet: 3''300RFOutlet: 4''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **3** |
| **FOR 400-PSV-3503A/3503B 400-PSV-3603A-3603B** | | | | |
| **97** | **Disc insert  MODEL PSV 3K4 JBS-E25-S-KS/N: 11-06877-11-06878Inlet: 3''300RFOutlet: 4''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **98** | **Spring  MODEL PSV 3K4 JBS-E25-S-KS/N: 11-06877-11-06878Inlet: 3''300RFOutlet: 4''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **99** | **Disc holder  MODEL PSV 3K4 JBS-E25-S-KS/N: 11-06877-11-06878Inlet: 3''300RFOutlet: 4''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **100** | **Bellows  MODEL PSV 3K4 JBS-E25-S-KS/N: 11-06877-11-06878Inlet: 3''300RFOutlet: 4''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **101** | **Gasket kit  MODEL PSV 3K4 JBS-E25-S-KS/N: 11-06877-11-06878Inlet: 3''300RFOutlet: 4''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **FOR 200-PSV-1202/1203 200-PSV-1502/2303 400-PSV-1210** | | | | |
| **102** | **Disc insert  MODEL PSV 9511012E-25-STMS/N: 11-06789Inlet: 3/4''300RFOutlet: 1''150RF set pressure: 35KG/CM2G** | | **ROOM** | **2** |
| **103** | **Spring  MODEL PSV 9511012E-25-STMS/N: 11-06789Inlet: 3/4''300RFOutlet: 1''150RF set pressure: 35KG/CM2G** | | **ROOM** | **2** |
| **104** | **O.ring kit  MODEL PSV 9511012E-25-STMS/N: 11-06789Inlet: 3/4''300RFOutlet: 1''150RF set pressure: 35KG/CM2G** | | **ROOM** | **2** |
| **105** | **Disc holder  MODEL PSV 9511012E-25-STMS/N: 11-06789Inlet: 3/4''300RFOutlet: 1''150RF set pressure: 35KG/CM2G** | | **ROOM** | **2** |
| **FOR 400-PSV-4201A/4201B** | | | | |
| **106** | **Disc insert  MODEL PSV 1E2 JBS-E-15-KS/N: 11-06891-11-06892Inlet: 1''150RFOutlet: 2''150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **107** | **Spring  MODEL PSV 1E2 JBS-E-15-KS/N: 11-06891-11-06892Inlet: 1''150RFOutlet: 2''150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **108** | **Gasket kit  MODEL PSV 1E2 JBS-E-15-KS/N: 11-06891-11-06892  Inlet: 1''150RF  Outlet: 2''150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **109** | **Bellows tailpiece  MODEL PSV 1E2 JBS-E-15-KS/N: 11-06891-11-06892Inlet: 1''150RFOutlet: 2''150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **110** | **Disc holder  MODEL PSV 1E2 JBS-E-15-KS/N: 11-06891-11-06892Inlet: 1''150RFOutlet: 2''150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **FOR 400-PSV-1207/3302/3303 600-PSV-6802** | | | | |
| **111** | **Disc insert  MODEL PSV BP513011BS/N: 11-06786Inlet: 0.75''150RFOutlet: 1.5''150RF set pressure: 13.5KG/CM2G** | | **ROOM** | **2** |
| **112** | **O.ring kit  MODEL PSV BP513011BS/N: 11-06786Inlet: 0,75''150RFOutlet: 1,5''150RF set pressure: 13.5KG/CM2G** | | **ROOM** | **2** |
| **113** | **Spring  MODEL PSV BP513011BS/N: 11-06786Inlet: 0.75''150RFOutlet: 1.5''150RF set pressure: 13.5KG/CM2G** | | **ROOM** | **2** |
| **114** | **Disc holder  MODEL PSV BP513011BS/N: 11-06786Inlet: 0.75''150RFOutlet: 1.5''150RF set pressure: 13.5KG/CM2G** | | **ROOM** | **2** |
| **FOR 400-PSV-1603A/1603B/1603C** | | | | |
| **115** | **Disc insert  MODEL PSV BP513011BS/N: 11-06790-1106792Inlet: 0.75''150RFOutlet: 1''150RF set pressure: 9.5KG/CM2G** | | **ROOM** | **2** |
| **116** | **Spring  MODEL PSV BP513011BS/N: 11-06790-1106792Inlet: 0.75''150RFOutlet: 1''150RF set pressure: 9.5KG/CM2G** | | **ROOM** | **2** |
| **117** | **O.ring kit  MODEL PSV BP513011BS/N: 11-06790-1106792Inlet: 0.75''150RFOutlet: 1''150RF set pressure: 9.5KG/CM2G** | | **ROOM** | **2** |
| **118** | **Disc Holder  MODEL PSV BP513011BS/N: 11-06790-1106792Inlet: 0.75''150RFOutlet: 1''150RF set pressure: 9.5KG/CM2G** | | **ROOM** | **2** |
| **FOR 400-PSV-1801A-1801B** | | | | |
| **119** | **Disc Insert  MODEL PSV 1.5G3 JBS-E32-KS/N: 11-06805-11-0680Inlet: 1.5''150RFOutlet: 3''150RF set pressure: 16KG/CM2G** | | **ROOM** | **2** |
| **120** | **Spring  MODEL PSV 1.5G3 JBS-E32-KS/N: 11-06805-11-0680Inlet: 1.5''150RFOutlet: 3''150RF set pressure: 16KG/CM2G** | | **ROOM** | **2** |
| **121** | **Gasket kit  MODEL PSV 1.5G3 JBS-E32-KS/N: 11-06805-11-0680Inlet: 1,5''150RFOutlet: 3''150RF set pressure: 16KG/CM2G** | | **ROOM** | **2** |
| **122** | **Bellows tailpiece  MODEL PSV 1.5G3 JBS-E32-KS/N: 11-06805-11-0680Inlet: 1.5''150RFOutlet: 3''150RF set pressure: 16KG/CM2G** | | **ROOM** | **2** |
| **FOR 400-PSV-1901A-1901B/2001A/2001B/2101A/2101B - 400-PSV-2201A-2201B/2301A/2301B/2401A/2401B** | | | | |
| **123** | **Disc insert  MODEL PSV 3K4 JBS-E12-KS/N: 11-06807-11-06808Inlet: 3''150RFOutlet: 4''150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **3** |
| **124** | **Spring  MODEL PSV 3K4 JBS-E12-KS/N: 11-06807-11-06808Inlet: 3''150RFOutlet: 4''150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **3** |
| **125** | **Disc holder  MODEL PSV 3K4 JBS-E12-KS/N: 11-06807-11-06808Inlet: 3''150RFOutlet: 4''150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **3** |
| **126** | **Bellows  MODEL PSV 3K4 JBS-E12-KS/N: 11-06807-11-06808Inlet: 3''150RFOutlet: 4''150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **3** |
| **127** | **Gasket kit  MODEL PSV 3K4 JBS-E12-KS/N: 11-06807-11-06808Inlet: 3''150RFOutlet: 4''150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **3** |
| **FOR 400-PSV-1902A-1902B** | | | | |
| **128** | **Disc insert  MODEL PSV 1.5 JBS-E22-K-SPLS/N: 11-06809-11-06810Inlet: 1.5''150RFOutlet: 3''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **129** | **Spring  MODEL PSV 1.5 JBS-E22-K-SPLS/N: 11-06809-11-06810Inlet: 1.5''150RFOutlet: 3''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **130** | **Disc holder  MODEL PSV 1.5 JBS-E22-K-SPLS/N: 11-06809-11-06810Inlet: 1.5''150RFOutlet: 3''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **131** | **Bellows  MODEL PSV 1.5 JBS-E22-K-SPLS/N: 11-06809-11-06810Inlet: 1.5''150RFOutlet: 3''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **132** | **Gasket kit  MODEL PSV 1.5 JBS-E22-K-SPLS/N: 11-06809-11-06810Inlet: 1.5''150RFOutlet: 3''150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **PDR FOR VALVE PSV 44310T810/S1 UNIT:701-103-1091** | | | | |
| **133** | **Piston seat  MODEL PSV N°: 44310T810/S1Const: TYCO** | | **ROOM** | **6** |
| **134** | **Seat  MODEL PSV No: 44310T810/S1Const: TYCO** | | **ROOM** | **6** |
| **135** | **Linear seat  MODEL PSV N°: 44310T810/S1Const: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 1,5H3 -JBS-E-15-K UNIT:701-103-1091** | | | | |
| **136** | **Disc holder  MODEL PSV No.: 1.5H3 -JBS-E-15-K Const: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 1.5H3 JLT-E-15-E UNIT:701-103-1091** | | | | |
| **137** | **Disc holder  MODEL PSV No.: 1.5H3 JLT-E-15-EConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 1,5F2 JLT-JOS-E-36-K UNIT:31-11-10-700** | | | | |
| **138** | **Disc holder  MODEL PSV No.: 1.5F2 JLT-JOS-E-36-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 1,5G3 JLT-JOS-E-15-K UNIT:31-11-10-700** | | | | |
| **139** | **Disc holder  MODEL PSV No.: 1.5G3 JLT-JOS-E-15-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 6Q8 JBS-E-16-K UNIT:31-11-10-700** | | | | |
| **140** | **Disc holder  MODEL PSV N°: 6Q8 JBS-E-16-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 2J3 JBS-E-15-K UNIT:31-11-10-700** | | | | |
| **141** | **Disc holder  MODEL PSV No.: 2J3 JBS-E-15-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 4P6 JLT-JBS-E-15-K UNIT:31-11-10-700** | | | | |
| **142** | **Disc holder  MODEL PSV N°: JLT-JBS-E-15-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 1D2 JLT-JOS-E-35-K UNIT:31-11-10-700** | | | | |
| **143** | **Disc holder  MODEL PSV N°: 1D2 JLT-JOS-E-35-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 3K4 JBS-E-15-E UNIT:31-11-10-700** | | | | |
| **144** | **Disc holder  MODEL PSV N°: 3K4 JBS-E-15-EConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR PSV VALVE 1.5H JLT-JBS-E-15-K UNIT:31-11-10-700** | | | | |
| **145** | **Disc holder  MODEL PSV No.: 1.5H JLT-JBS-E-15-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 2J3 JOS-E-15-E UNIT:1081-700-701-100** | | | | |
| **146** | **Disc holder  MODEL PSV N°: 2J3 JOS-E-15-EConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 3L4 JOS-E-15-E UNIT:1081-700-701-100** | | | | |
| **147** | **Disc insert  MODEL PSV No.: 3L4 JOS-E-15-EConst: TYCO** | | **ROOM** | **6** |
| **148** | **O-ring  MODEL PSV N°: 3L4 JOS-E-15-EConst: TYCO** | | **ROOM** | **6** |
| **149** | **Cap gasket  MODEL PSV N°: 3L4 JOS-E-15-EConst: TYCO** | | **ROOM** | **6** |
| **150** | **Gasket guide  MODEL PSV N°: 3L4 JOS-E-15-EConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 8T10 JOS-HE-45-C UNIT:1070-1051-701** | | | | |
| **151** | **Disc holder  MODEL PSV N°: 8T10 JOS-HE-45-CConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 8T210 JOS-HE-15-C-SPL UNIT:1070-1051-701** | | | | |
| **152** | **Disc insert  MODEL PSV N°: 8T210 JOS-HE-15-C-SPLConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR PSV VALVE P/UNITE:10-11-100-30-31-200-1120-1121-1060-1070-400-500-900-700-701-702-703-1082-1081-62** | | | | |
| **153** | **Bellows  Part No: S91328MODEL: 2J3 JBS-E-15-K/E-12-EConst: TYCO** | | **ROOM** | **10** |
| **154** | **Bellows  Part No: S91326MODEL: 1.5G3 JBS-E-25-KConst: TYCO** | | **ROOM** | **10** |
| **155** | **Bellows  Part No: S91772MODEL: 6Q8 JBS-E-16-K/E-35-KConst: TYCO** | | **ROOM** | **10** |
| **156** | **Bellows  Part No: S91341MODEL: 8T10 JBS-E-45-KConst: TYCO** | | **ROOM** | **10** |
| **157** | **Bellows  Part No: S91741MODEL: 1.5H3 JLT-JBS-E-15-K and JBS-EConst: TYCO** | | **ROOM** | **10** |
| **PDR FOR VALVE PSV MODEL 1E2 JOS-E-35-K UNIT:1070-1051-701** | | | | |
| **158** | **Disc holder  MODEL PSV 1E2 JOS-E-35-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR PSV VALVE MODEL 26305-810/S1 UNIT:1070-1051-701** | | | | |
| **159** | **Blowdown seal  MODEL PSV 26305-810/S1N°24 on drawingConst: TYCO** | | **ROOM** | **6** |
| **160** | **Bushing seal  MODEL PSV 26305-810/S1N°21 on drawingConst: TYCO** | | **ROOM** | **6** |
| **161** | **Piston seal  MODEL PSV 26305-810/S1N°18 on drawing  Const: TYCO** | | **ROOM** | **6** |
| **162** | **Blowdown  MODEL PSV 26305-810/S1N°16 on drawingConst: TYCO** | | **ROOM** | **6** |
| **163** | **Spring  MODEL PSV 26305-810/S1N°10 on drawingConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR UNIT: 700-701-11-1051-1071-1061-1031-1081-31-1082-1060-100** | | | | |
| **164** | **Spring  Part No.SX36372Model No.: 8T10 JBS-E-45-KConst: TYCO** | | **ROOM** | **10** |
| **PDR FOR UNIT: 100-11-1082-10 PSV 44305T810/S1** | | | | |
| **165** | **O-ring kit  Model No.: 44305T810/S1Const: TYCO** | | **ROOM** | **6** |
| **FOR 400-PSV-3502A/3502B** | | | | |
| **166** | **Disc holder  For PSV Model: 1.5G3 JBS-E-35-S-KS/N: 11-06875-1106876Inlet: 1.5'' 300RFOutlet: 3'' 150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **167** | **Disc insert  For PSV Model: 1.5G3 JBS-E-35-S-KS/N: 11-06875-1106876Inlet: 1.5'' 300RFOutlet: 3'' 150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **168** | **Spring  For PSV Model: 1.5G3 JBS-E-35-S-KS/N: 11-06875-1106876Inlet: 1.5'' 300RFOutlet: 3'' 150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **169** | **Gasket kit  For PSV Model: 1.5G3 JBS-E-35-S-KS/N: 11-06875-1106876Inlet: 1.5'' 300RFOutlet: 3'' 150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **170** | **Bellows  For PSV Model: 1.5G3 JBS-E-35-S-KS/N: 11-06875-1106876Inlet: 1.5'' 300RFOutlet: 3'' 150RF set pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **For 100-PSV-2201200-PSV-1801A/1801B 400-PSV-3401A-3401/B 701-PSv-1101A/1101B 703-PSV-1101A** | | | | |
| **171** | **Disc insert  For PSV Model: 3L4 JBS-E-15-S-KS/N: 11-06875-1106872  Inlet: 3'' 300RF  Outlet: 4'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **3** |
| **172** | **Spring  For PSV Model: 3L4 JBS-E-15-S-KS/N: 11-06875-1106872Inlet: 3'' 300RFOutlet: 4'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **3** |
| **FOR 400-PSV-2801A/2801B** | | | | |
| **173** | **Disc insert  For PSV Model: 4M6 JBS-E-12-KS/N: 11-06853-11-06854Inlet: 4'' 300RFOutlet: 6'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **174** | **Spring  For PSV Model: 4M6 JBS-E-12-KS/N: 11-06853-11-06854Inlet: 4'' 300RFOutlet: 6'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **175** | **Disc holder  For PSV Model: 4M6 JBS-E-12-KS/N: 11-06853-11-06854Inlet: 4'' 300RFOutlet: 6'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **176** | **Spindle  For PSV Model: 4M6 JBS-E-12-KS/N: 11-06853-11-06854Inlet: 4'' 300RFOutlet: 6'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **FOR 400-PSV-3101A/3102A 400-PSV-3001A/3001B** | | | | |
| **177** | **Spring  For PSV Model: 2J3 JBS-E-12-KS/N: 11-06862Inlet: 2'' 150RFOutlet: 3'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **178** | **Disc holder  For PSV Model: 2J3 JBS-E-12-KS/N: 11-06862Inlet: 2'' 150RFOutlet: 3'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **179** | **Spindle  For PSV Model: 2J3 JBS-E-12-KS/N: 11-06862Inlet: 2'' 150RFOutlet: 3'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **180** | **Disc insert  For PSV Model: 2J3 JBS-E-12-KS/N: 11-06862Inlet: 2'' 150RFOutlet: 3'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **FOR 400-PSV-3101A/3101A 400-PSV-3002A/3002B** | | | | |
| **181** | **Disc holder  For PSV Model: 56605-810/S1S/N: 11-06793-11-06796Inlet: 8'' 150RFOutlet: 10'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **FOR 10-PSV-1114/11-PSV-2114 100-PSv-2401A/2401B 400-PSV-3801A/3801B/3802A** | | | | |
| **182** | **Disc insert  For PSV Model: 2J3 JBS-E-15-KS/N: 11-06887-11-06888Inlet: 2'' 150RFOutlet: 3'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **3** |
| **183** | **Spring  For PSV Model: 2J3 JBS-E-15-KS/N: 11-06887-11-06888Inlet: 2'' 150RFOutlet: 3'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **3** |
| **184** | **Disc holder  For PSV Model: 2J3 JBS-E-15-KS/N: 11-06887-11-06888Inlet: 2'' 150RFOutlet: 3'' 150RF set pressure: 3.5KG/CM2G** | | **ROOM** | **3** |
| **PDR for unit: 200-PSV-1501A/B** | | | | |
| **185** | **Spring: SST 316  For PSV: 6" inlet 150RF OUTLET: 8" 150RFModel: 950608RS** | | **ROOM** | **2** |
| **186** | **Nozzle: SST SA479-316  For PSV: 6" inlet 150RF OUTLET: 8" 150RFModel: 950608RS** | | **ROOM** | **2** |
| **187** | **Spindle: SST SA479-304  For PSV: 6" inlet 150RF OUTLET: 8" 150RFModel: 950608RS** | | **ROOM** | **2** |
| **PDR for unit: 200-PSV-1204** | | | | |
| **188** | **Spring (KIT)  For PSV: 4" inlet 300RF OUTLET: 6" 150RFModel: 4N6 JLT-JBS-E-25-K- Part N°:SX36267-103157** | | **ROOM** | **1** |
| **189** | **Disc Insert: SST SA479-316  For PSV: 4" 300RF inlet OUTLET: 6" 150RFModel: 4N6 JLT-JBS-E-25-K Part N°: 145870** | | **ROOM** | **1** |
| **190** | **Disc Holder: SST SA351-CF3M  For PSV: 4" inlet 300RF OUTLET: 6" 150RFModel: 4N6 JLT-JBS-E-25-K Part N°: 146384** | | **ROOM** | **1** |
| **PDR for unit: 200-PSV-1101A/B** | | | | |
| **191** | **Disc Insert: SST SA479-316  For PSV: 3/4" inlet 150RF OUTLET: 1" 150RFModel: BP513011EPart N°: 122598** | | **ROOM** | **2** |
| **192** | **Disc Holder: SST SA479-316  For PSV: 3/4" inlet 150RF OUTLET: 1" 150RFModel: BP513011E Part N°: 140945** | | **ROOM** | **2** |
| **PDR for unit: 200-PSV-1902A/B** | | | | |
| **193** | **Spring (200-PSV-1101A,SN:06457)  For PSV: 3/4" inlet 150RF OUTLET: 1" 150RFModel: BP513011EPart N°: X09835** | | **ROOM** | **2** |
| **194** | **Spring (KIT)  For PSV: 1.5" inlet 150RF OUTLET: 3" 150RFModel: 1.5H3 JBS-E-15-E Part N°:SX36073-102713** | | **ROOM** | **2** |
| **195** | **Disc Insert: SST SA479-316  For PSV: 1.5" inlet 150RF OUTLET: 3" 150RFModel: 1.5H3 JBS-E-15-E Part N°: 136980** | | **ROOM** | **2** |
| **196** | **Disc Holder: SST SA351-CF3M  For PSV: 1.5" inlet 150RF OUTLET: 3" 150RFModel: 1.5H3 JBS-E-15-E Part N°: 147195** | | **ROOM** | **2** |
| **PDR for unit: 200-PSV-1901A/B** | | | | |
| **197** | **Spring (KIT)  For PSV: inlet 4" 150RF OUTLET: 6" 150RFModel: 4M6 JBS-E-15-E** | | **ROOM** | **2** |
| **198** | **Disc Insert: SST SA479-316  For PSV: 4" 150RF inlet OUTLET: 6" 150RFModel: 4M6 JBS-E-15-E** | | **ROOM** | **2** |
| **199** | **Disc Holder: SST SA351-CF3M  For PSV: 4" inlet 150RF OUTLET: 6" 150RFModel: 4M6 JBS-E-15-E** | | **ROOM** | **2** |
| **PDR for unit: 200-PSV-3002** | | | | |
| **200** | **Spring: Chrome steel  For PSV: inlet 6" 600RF OUTLET: 8" 150RFModel: 6Q8 JOS-HE-45-C** | | **ROOM** | **1** |
| **201** | **Disc Insert: ASME SA479  Type: 316For PSV: 6" 600RF inlet OUTLET: 6" 150RFModel: 6Q8 JOS-HE-45-C** | | **ROOM** | **1** |
| **202** | **Sprindle: 416 SST  For PSV: 6" inlet 600RF OUTLET: 8" 150RFModel: 6Q8 JOS-HE-45-C** | | **ROOM** | **1** |
| **PDR for unit: 200-PSV-2002A/2001A/2001B** | | | | |
| **203** | **Spring steel  For PSV: inlet 3" 300RF OUTLET: 4" 150RFModel: 3K4 JBS-E36-SPL TYPE K** | | **ROOM** | **3** |
| **204** | **Disc Insert: ASME SA479  Type: 316For PSV: 3" 300RF inlet OUTLET: 4" 150RFModel: 3K4 JBS-E36-SPL TYPE K** | | **ROOM** | **3** |
| **205** | **Disc Holder: 316L SST  For PSV: 3" 300RF inlet OUTLET: 4" 150RFModel: 3K4 JBS-E36-SPL TYPE K** | | **ROOM** | **3** |
| **PDR for PSV valve FOR unit: 10-11-100-30-31-200-1120-1121-1060-170-400-500-900-700-701-702-703-1082-10181-62** | | | | |
| **206** | **Bellows ( Bellows )  Part N° S91331Model: 4M6JLT-JBS-E-15-K and JBS-E** | | **ROOM** | **10** |
| **207** | **Bellows ( Bellows )  Part N° S91773 Model: 6R10-JBS-E-35-KConst : TYCO** | | **ROOM** | **10** |
| **208** | **Bellows (Bellows)  Part N° S91335Model: 4P6JLT-JBS-E-15-K and JBS-EConst: TYCO** | | **ROOM** | **10** |
| **209** | **Bellows (Bellows)  Part N° S91325Model: 1,5F2JLT-JBS-E-15-K and JBS-EConst: TYCO** | | **ROOM** | **10** |
| **210** | **Bellows (Bellows)  Part N° S91740Model: 1E2JLT-JBS-E-15-K and JBS-EConst: TYCO** | | **ROOM** | **10** |
| **211** | **Bellows (Bellows)  Part N° S91743Model: 3L4JLT-JBS-E-15-K and JBS-EConst: TYCO** | | **ROOM** | **10** |
| **PDR for PSV valve 9511012E unit: 700-701** | | | | |
| **212** | **Spring Steel  PSV Model: 9511012E** | | **ROOM** | **6** |
| **213** | **Disc Holder  Model: 9511012E** | | **ROOM** | **6** |
| **214** | **O-Ring Kit  Model: 9511012E** | | **ROOM** | **6** |
| **PDR for valve PSV 1E2 JOS-E-35-N2-K unit: 700-701** | | | | |
| **215** | **Disc Holder  PSV Model: 1E2 JOS-E-35-N2-K** | | **ROOM** | **6** |
| **216** | **O-Ring kit  Model: 1E2 JOS-E-35-N2-K** | | **ROOM** | **6** |
| **PDR for PSV valve 9511011E unit: 700-701** | | | | |
| **217** | **Disc Holder  PSV Model: 9511011E** | | **ROOM** | **20** |
| **218** | **O-Ring Kit  Model: 9511011E** | | **ROOM** | **20** |
| **219** | **Spring  PSV Model: 9511011E** | | **ROOM** | **20** |
| **PDR for valve PSV 1D2 JOS-E-35-K unit: 10-700-701** | | | | |
| **220** | **O-Ring Kit  Model: 1D2 JOS-E-35-K** | | **ROOM** | **6** |
| **221** | **Disc Holder  PSV Model: 1D2 JOS-E-35-K** | | **ROOM** | **6** |
| **PDR for valve PSV 1.5F2 JOS-E-35-K unit: 700-701** | | | | |
| **222** | **Spring (KIT)  Model: 1,5F2 JOS-E-35-K** | | **ROOM** | **6** |
| **223** | **Disc Holder  PSV Model: 1.5F2 JOS-E-35-K** | | **ROOM** | **6** |
| **224** | **O-Ring Kit  Model: 1.5F2 JOS-E-35-K** | | **ROOM** | **6** |
| **PDR for valve PSV 4M6 JOS-E-35-M4-K unit: 700-701** | | | | |
| **225** | **Spring (KIT)  Model: 4M6 JOS-E-35-M4-K** | | **ROOM** | **6** |
| **226** | **Disc Holder  Model: 4M6 JOS-E-35-M4-K** | | **ROOM** | **6** |
| **227** | **O-Ring Kit  Model: 4M6 JOS-E-35-M4-K** | | **ROOM** | **6** |
| **PDR for valve PSV 3J4 JOS-E-35-M4-K unit: 700-701** | | | | |
| **228** | **Spring (KIT)  PSV Model: 3J4 JOS-E-35-M4-K** | | **ROOM** | **6** |
| **229** | **Disc Holder  PSV Model: 3J4 JOS-E-35-M4-K** | | **ROOM** | **6** |
| **230** | **O-Ring Kit  Model: 3J4 JOS-E-35-M4-K** | | **ROOM** | **6** |
| **PDR for unit: 100-11-1082-10 PSV 3K4 JBS-E-15-E** | | | | |
| **231** | **O-Ring Kit  Model: 3K4 JBS-E-15-E** | | **ROOM** | **6** |
| **PDR for unit: 100-11-1082-10 PSV 1.5G3 JBS-E-15-K** | | | | |
| **232** | **Spring (KIT)  Model: 1.5G3 JBS-E-15-K Part No: SX36081-102713** | | **ROOM** | **6** |
| **233** | **Disc Holder  Model: 1.5G3 JBS-E-15-K Part No: 147156** | | **ROOM** | **6** |
| **234** | **O-Ring Kit  Model: 1.5G3 JBS-E-15-K** | | **ROOM** | **6** |
| **PDR for unit: 63/1070/1031/1082/1081 PSV 9511111B** | | | | |
| **237** | **Spring  Model: 9511111B** | | **ROOM** | **3** |
| **238** | **Disc Holder  Model: 9511111B** | | **ROOM** | **3** |
| **239** | **O-Ring kit  Model: 9511111B** | | **ROOM** | **3** |
| **PDR for valve PSV 2H3 JOS-E-35-K unit: 700-701** | | | | |
| **240** | **Spring  PSV Model: 2H3 JOS-E-35-K** | | **ROOM** | **6** |
| **241** | **Disc Holder  PSV Model: 2H3 JOS-E-35-K** | | **ROOM** | **6** |
| **242** | **O-Ring Kit  Model: 2H3 JOS-E-35-K** | | **ROOM** | **6** |
| **PDR for unit: 100-11-1082-10 PSV 46305-810/S1** | | | | |
| **243** | **Piston Seal  PSV Model: 46305-810/S1** | | **ROOM** | **6** |
| **244** | **Seat  Model: 46305-810/S1** | | **ROOM** | **6** |
| **245** | **Linear Seal  PSV Model: 46305-810/S1** | | **ROOM** | **6** |
| **246** | **Spring  Model: 46305-810/S1** | | **ROOM** | **6** |
| **247** | **Disc Holder  Model: 46305-810/S1** | | **ROOM** | **6** |
| **248** | **O-Ring Kit  Model: 46305-810/S1** | | **ROOM** | **6** |
| **PDR for unit: 100-200-1080-1051-600-63-1031-11 PSV 9511011E** | | | | |
| **249** | **Seat  Model: 9511011E** | | **ROOM** | **20** |
| **250** | **Piston Seal  Model: 9511011E** | | **ROOM** | **20** |
| **251** | **Linear Seal  Model: 9511011E** | | **ROOM** | **20** |
| **PDR for unit: 100-1080-1051-600-63-1031-11 PSV 9511011B** | | | | |
| **252** | **Seat  Model: 9511011B** | | **ROOM** | **50** |
| **253** | **Piston Seal  Model: 9511011B** | | **ROOM** | **50** |
| **254** | **Linear Seal  Model: 9511011B** | | **ROOM** | **50** |
| **255** | **Spring  Model: 9511011B Part No: X09745** | | **ROOM** | **50** |
| **256** | **Disc Holder  Model: 9511011B Part No: 121392** | | **ROOM** | **50** |
| **257** | **O-Ring Kit  Model: 9511011B** | | **ROOM** | **50** |
| **PDR for unit: 100-11-1082-10 PSV 6Q8 JBS-E15-K** | | | | |
| **258** | **Spring  Model: 6Q8 JBS-E15-SPL TYPE K** | | **ROOM** | **6** |
| **259** | **Disc Holder  Model: 6Q8 JBS-E15-SPL TYPE K** | | **ROOM** | **6** |
| **260** | **O-Ring Kit  Model: 6Q8 JBS-E15-SPL TYPE K** | | **ROOM** | **6** |
| **PDR for unit: 702-PSV-1601A** | | | | |
| **261** | **Disc Holder: 316L SST  N°5 on drawingModel: 3K4 JOS-E-37-S SPL TYPE E** | | **ROOM** | **1** |
| **262** | **Disc Insert  N°8 on drawing: ASME SA479 TYPE 316 Model: 3K4 JOS-E-37-S SPL TYPE E** | | **ROOM** | **1** |
| **263** | **Gasket (Guide)  N°28 on drawing Soft annealed 316 SSTModel: 3K4 JOS-E-37-S SPL TYPE E** | | **ROOM** | **1** |
| **264** | **Spring: Inconel X-750  N°18 on drawing Model: 3K4 JOS-E-37-S SPL TYPE E** | | **ROOM** | **1** |
| **265** | **Nozzle: ASME SA351 GR-CF8M  N°2 on drawing Model: 3K4 JOS-E-37-S SPL TYPE E** | | **ROOM** | **1** |
| **PDR for unit: 200-PSV-1503** | | | | |
| **266** | **Spring: Chrome Steel  For PSV: Inlet 1" 150RF Outlet: 2" 150RFModel: 1D2 JBS-E-15-SPL TYPE K** | | **ROOM** | **2** |
| **267** | **Nozzle: ASME SA351 GR-CF8M  For PSV: Inlet 1" 150RF Outlet: 2" 150RFModel: 1D2 JBS-E-15-SPL TYPE K** | | **ROOM** | **2** |
| **268** | **Disc Holder: SST361L  For PSV: Inlet 1" 150RF Outlet: 2" 150RFModel: 1D2 JBS-E-15-SPL TYPE K** | | **ROOM** | **2** |
| **PDR for unit: 200-PSV-2501 A/B** | | | | |
| **269** | **Bellows: Incnel 625  For PSV: Inlet 4" 150RF Outlet: 6" 150RFModel: 4M6 JBS-E-15-K** | | **ROOM** | **2** |
| **270** | **Nozzle: ASME SA351 GR-CF8M  For PSV: Inlet 4" 150RF Outlet: 6" 150RFModel: 4M6 JBS-E-15-K** | | **ROOM** | **2** |
| **PDR for unit: 500-PSV-1801A/B** | | | | |
| **271** | **Bellows: Incnel 625  For PSV: Inlet 4" 150RF Outlet: 6" 150RFModel: 4N6 JBS-E-15-K** | | **ROOM** | **2** |
| **272** | **Nozzle  For PSV: Inlet 4" 150RF Outlet: 6" 150RFModel: 4N6 JBS-E-15-K** | | **ROOM** | **2** |
| **PDR for unit: 200-PSV-1702 A/B** | | | | |
| **273** | **Spring (KIT)  For PSV: Inlet 3" 150RF Outlet: 4" 150RFModel: 3K4 JBS-E-15-K** | | **ROOM** | **2** |
| **274** | **Nozzle: SST SA351-CF8M  For PSV: Inlet 3" 150RF Outlet: 4" 150RFModel: 3K4 JBS-E-15-K** | | **ROOM** | **2** |
| **PDR for unit: 200-PSV-1801A/B** | | | | |
| **275** | **Spring (KIT)  For PSV: Inlet 3" 150RF Outlet: 4" 150RFModel: 3L4 JBS-E-15-K** | | **ROOM** | **2** |
| **276** | **Nozzle: SST SA351-CF8M  For PSV: Inlet 8" 300RF Outlet: 10" 300RFModel: 3L4 JBS-E-15-K** | | **ROOM** | **2** |
| **PDR for unit: 200-PSV-2301A/B** | | | | |
| **277** | **Nozzle: SST SA351-CF3M  For PSV: Inlet 8" 300RF Outlet: 10" 300RFModel: 8T10 JBS-E-15-K** | | **ROOM** | **2** |
| **278** | **Spring (KIT)  For PSV: Inlet 8" 300RF Outlet: 10" 300RFModel: 8T10 JBS-E-15-K** | | **ROOM** | **2** |
| **PDR for unit: 200-PSV-2102A/B** | | | | |
| **279** | **Spring (KIT)  For PSV: Inlet 6" 150RF Outlet: 8" 150RFModel: 6R8 JBS-E-15-K** | | **ROOM** | **2** |
| **280** | **Disc Insert  For PSV: Inlet 6" 150RF Outlet: 8" 150RFModel: 6R8 JBS-E-15-K** | | **ROOM** | **2** |
| **281** | **Disc Holder  For PSV: Inlet 6" 150RF Outlet: 8" 150RFModel: 6R8 JBS-E-15-K** | | **ROOM** | **2** |
| **PDR for unit: 200-PSV-2005** | | | | |
| **282** | **Spring  For PSV: Inlet 3/4" 150RF Outlet: 1" 150RFModel: 9511812E Part N°: X09369** | | **ROOM** | **1** |
| **283** | **Disc Insert  For PSV: Inlet 3/4" 150RF Outlet: 1" 150RFModel: 9511812E Part N°: 121391** | | **ROOM** | **1** |
| **284** | **Disc Holder  For PSV: Inlet 3/4" 150RF Outlet: 1" 150RFModel: 9511812E Part N°: 125278** | | **ROOM** | **1** |
| **PDR for unit: 200-PSV-2004 A/B** | | | | |
| **285** | **Spring  For PSV: Inlet 3/4" 150RF Outlet: 1" 150RFModel: BP513812B** | | **ROOM** | **3** |
| **286** | **Disc Insert  For PSV: Inlet 3/4" 150RF Outlet: 1" 150RFModel: BP513812B** | | **ROOM** | **3** |
| **PDR for unit: 200-PSV-2901** | | | | |
| **287** | **Spindle: SST A479-316  For PSV: Inlet 3/4" 150RF Outlet: 1" 150RFModel: 81PS1S6A8A-4** | | **ROOM** | **1** |
| **288** | **Seat: See soft goods  For PSV: Inlet 3/4" 150RF Outlet: 1" 150RFModel: 81PS1S6A8A-4** | | **ROOM** | **1** |
| **289** | **Spring: SST SA479-316  For PSV: Inlet 3/4" 150RF Outlet: 1" 150RFModel: 81PS1S6A8A-4** | | **ROOM** | **1** |
| **PDR for unit: 200-PSV-2004 A/B** | | | | |
| **290** | **Disc Holder  For PSV: Inlet 3/4" 150RF Outlet: 1" 150RFModel: BP513812B** | | **ROOM** | **3** |
| **PDR for PSV valve model 45312D12/SA unit 1081-700-701-703-100** | | | | |
| **291** | **Seat liner  Model PSV 45312D12/SAN° 06 On Drawing** | | **ROOM** | **8** |
| **PDR for PSV valve model 44310H153/S1 unit 1081-700-701-100** | | | | |
| **292** | **Piston seal  Model PSV 44310H153/S1N° 13 On Drawing** | | **ROOM** | **8** |
| **293** | **Seat  Model PSV 44310H153/S1N° 7 On Drawing** | | **ROOM** | **8** |
| **294** | **Linear seal  Model PSV 44310H153/S1N° 06 On Drawing** | | **ROOM** | **8** |
| **PDR for PSV valve model 1.5F2 JLT-JOS-E-15-E unit 10-1070-1051-701** | | | | |
| **295** | **Disc holder  Model PSV 1.5F2 JLT-JOS-E-15-E** | | **ROOM** | **6** |
| **PDR for PSV valve for unit 10-11-100-30-31-200-1120-1121-1060-1070-400-500-900-700-701-702-703-1082-1081-62** | | | | |
| **296** | **Bellows (Bellows) (EX:10-PSV-1858A/S ,SN:11-04900/04901)  Model: 3K4JLT-JBS-E-15-K Part N° S91742** | | **ROOM** | **10** |
| **297** | **Bellows (Bellows) (702-PSV-2001A ,SN:11-07509)  Model: 4N6JLT-JBS-E-15-N2-K and JBS-E Part N° S91332** | | **ROOM** | **10** |
| **PDR for unit: 200-PSV-2003A-2003B-2003C-2902-1103** | | | | |
| **298** | **Spring SST 316  For PSV: Inlet 3/4" 300RF Outlet: 1" 150RFModel: 81PS1S6B8A-4** | | **ROOM** | **6** |
| **299** | **Disc insert AST4140/ZN CO  For PSV: Inlet 3/4" 300RF Outlet: 1" 150RFModel: 81PS1S6B8A-4** | | **ROOM** | **6** |
| **300** | **Spindle SST A479-316  For PSV: Inlet 3/4" 300RF Outlet: 1" 150RFModel: 81PS1S6B8A-4** | | **ROOM** | **6** |
| **PDR for unit: 700-701-11-1051-1071-1061-1031-1081-31-1082-1060-100** | | | | |
| **301** | **Disc insert (Ex:100-PSV- 2204, SN:11-05722)  Model: 1.5F2 JBS-E-15-SPL TYPE KPart No: 136978** | | **ROOM** | **10** |
| **302** | **Disc insert (EX:1051-PSV-1204A/ D , SN:11-07648/49)  Model: 8T10JOS-HE-35-CPart No: 145874** | | **ROOM** | **10** |
| **303** | **Spring (KIT) (EX:10-PSV-60A , SN:11-28857)  Model: 6Q8 JBS-E16-K Part No:SX07808** | | **ROOM** | **10** |
| **304** | **Spring (KIT) (EX:10-PSV-38A/S , SN:11-04915/16)  Model: 8T10 JBS-E45-K Part No: SX36056** | | **ROOM** | **10** |
| **PDR for PSV valve 9511012B-SPL unit 701-703-1091** | | | | |
| **305** | **Spring  Model: 9511012B-SPL** | | **ROOM** | **6** |
| **306** | **Disc holder  Model: 9511012B-SPL** | | **ROOM** | **6** |
| **307** | **O-Ring Kit  Model: 9511012B-SPL** | | **ROOM** | **6** |
| **PDR for valve PSV 1.5F2 JBS-E16-SPL TYPE K unit 701-703-1091** | | | | |
| **308** | **Tailpiece  Model: 1.5F2 JBS-E16-K** | | **ROOM** | **6** |
| **309** | **Disc insert  Model: 1.5F2 JBS-E16-K** | | **ROOM** | **6** |
| **310** | **Bellows  Model: 1.5F2 JBS-E16-M** | | **ROOM** | **6** |
| **311** | **Disc holder  Model: 1.5F2 JBS-E16-K** | | **ROOM** | **6** |
| **PDR for valve PSV 1.5 G3 JBS-E-25-K unit 701-703-1091** | | | | |
| **312** | **Disc holder  Model: 1.5G3 JBS-E-25-K** | | **ROOM** | **6** |
| **PDR for valve PSV 6R10 JBS-E-35-K unit 31-11-10-700** | | | | |
| **313** | **Disc holder  Model: 6R10 JBS-E-35-K** | | **ROOM** | **6** |
| **PDR for valve PSV 4M6 JBS-E-15-N2-K unit 31-11-10-700** | | | | |
| **314** | **Disc holder  Model: 4M6 JBS-E-15-N2-K** | | **ROOM** | **6** |
| **PDR for PSV valve 4L6-JOS-HE-37-SPL TYPE C unit 31-11-10-700** | | | | |
| **315** | **Disc holder  Model: 4L6-JOS-HE-37-SPL TYPE C** | | **ROOM** | **6** |
| **PDR for PSV valve 3L4-JLT-JBS-E-15-K unit 31-11-10-700** | | | | |
| **316** | **Disc holder  Model: 3L4-JLT-JBS-E-15-K** | | **ROOM** | **6** |
| **PDR for valve PSV 1.5F2 JLT-JOS-E-35-K unit 31-11-10-700** | | | | |
| **317** | **Disc holder  Model: 1.5F2 JLT-JOS-E-35-K** | | **ROOM** | **6** |
| **PDR for valve PSV 6R10 JLT-JBS-E-45-K unit 31-11-10-700** | | | | |
| **318** | **Bushing  PSV Model: 6R10 JLT-JBS-E-45-SPL TYPE K** | | **ROOM** | **6** |
| **319** | **Disc holder  PSV Model: 6R10 JLT-JBS-E-45-SPL TYPE K** | | **ROOM** | **6** |
| **PDR for PSV valve 4P6-JBS-E-15-K unit 31-11-10-700** | | | | |
| **320** | **Disc holder  PSV Model: PSV 4P6-JBS-E-15-K** | | **ROOM** | **6** |
| **PDR for valve 1E2 JLT-JBS-E-15-K unit 30-31-11-10-700** | | | | |
| **321** | **Disc holder  PSV Model: 1E2 JLT-JBS-E-15-K** | | **ROOM** | **6** |
| **PDR for valve PSV 1.5G3 JBS-E-15-K** | | | | |
| **322** | **Disc holder  PSV Model: 1.5G3 JBS-E-15-K** | | **ROOM** | **6** |
| **PDR for valve PSV 8T10 JBS-E-15-N2-K unit 1081-700-701-702-100** | | | | |
| **323** | **Disc insert  PSV Model: 8T10 JBS-E-15-N2-K** | | **ROOM** | **6** |
| **324** | **Disc holder  PSV Model: 8T10 JBS-E-15-N2-K** | | **ROOM** | **6** |
| **PDR for PSV valve 8T10 JLT-JBS-E-15--K unit 1081-700-701-100** | | | | |
| **325** | **Disc holder  PSV Model: 8T10 JLT-JBS-E-15--K** | | **ROOM** | **6** |
| **PDR for valve PSV 1D2 JOS-E-35-E unit 1081-700-701-703-100** | | | | |
| **326** | **Disc holder  PSV Model: 1D2 JOS-E-35-E** | | **ROOM** | **6** |
| **PDR for PSV valve 45312D12/S1unit 1081-700-701-100** | | | | |
| **327** | **Piston Seat  PSV Model: 45312D12/S1 N° 13 On drawing** | | **ROOM** | **8** |
| **For 400-PSV-1903A-1903B/2003A/2003B/2103A/2103B 400-PSV-2203A-2203B/2203A/2303B/2403A/2403B** | | | | |
| **328** | **Disc Holder  PSV model: 3K4 JBS-E22-KS/N: 11-06811-11-06812Inlet: 3'' 300 RFOutlet: 4'' 150 RF Set Pressure: 10.5KG/CM2G** | | **ROOM** | **3** |
| **400-PSV-3602A/3602B; 400-PSV-1103/1104** | | | | |
| **329** | **Disc Insert  PSV Model: 1D2 JLT-JBS-E-35-KS/N: 11-06775Inlet: 1/2'' 300 RFOutlet: 2'' 150 RF Set Pressure: 27KG/CM2G** | |  | **2** |
| **330** | **Spring  PSV MODEL: 1D2 JLT-JBS-E-35-KS/N: 11-06775INLET: 1/2'' 300RFOUTLET:2'' 150RFSET PRESSURE: 27KG/CM2G** | |  | **2** |
| **331** | **DISC HOLDER  PSV MODEL: 1D2 JLT-JBS-E-35-KS/N: 11-06775Inlet: 1/2'' 300 RFOutlet: 2'' 150 RF Set Pressure: 27KG/CM2G** | |  | **2** |
| **332** | **Spindle  PSV Model: 1D2 JLT-JBS-E-35-KS/N: 11-06775Inlet: 1/2'' 300RFSet Pressure: 27KG/CM2G** | |  | **2** |
| **333** | **Disc Insert  PSV Model: 1D2 JLT-JBS-EK S/N: 11-06778INLET: 1/2'' 300RFOUTLET: 2'' 150RFSET PRESSURE: 11.8KG/CM2G** | |  | **3** |
| **334** | **Spring  PSV MODEL: 1D2 JLT-JBS-E-15-KS/N: 11-06778INLET: 1/2'' 300RFOUTLET:2'' 150RFSET PRESSURE: 11.8KG/CM2G** | |  | **3** |
| **335** | **Disc Holder  1D2 JLT-JBS-E-15-KS/N: 11-06778INLET: 1/2'' 300RFOUTLET: 2'' 150RFSET PRESSURE: 11.8KG/MG** | |  | **3** |
| **336** | **Spindle  1D2 JLT-JBS-E-15-KS/N: 11-06778INLET: 1/2'' 300RFOUTLET: 2'' 150RFSET PRESSURE: 11.8KG/CM2G** | |  | **3** |
| **400-PSV-1110** | | | | |
| **337** | **Disc Insert  PSV MODEL: 1.5F2 JLT-JBS-E-36-KS/N: 11-06920Inlet: 1/5'' 300 RFOutlet: 2'' 150 RF Set Pressure: 27KG/CM2G** | |  | **1** |
| **338** | **SPRING  PSV MODEL: 1.5F2 JLT-JBS-E-36-KS/N: 11-06920Inlet: 1/5'' 300 RFOutlet: 2'' 150 RF Set Pressure: 27KG/CM2G** | |  | **1** |
| **339** | **DISC HOLDER  PSV MODEL: 1.5F2 JLT-JBS-E-36-KS/N: 11-06920Inlet: 1/5'' 300RFOutlet: 2'' 150RFSet Pressure: 27KG/CM2G** | |  | **1** |
| **340** | **Spindle  PSV MODEL: 1.5F2 JLT-JBS-E-36-KS/N: 11-06920Inlet: 1/5'' 300RFOutlet: 2'' 150RFSet Pressure: 27KG/CM2G** | |  | **1** |
| **400-PSV-1202A/1202B 400-PSV-1203A** | | | | |
| **341** | **Disc Insert  PSV MODEL: 3L4 J-JBS-E-26-KS/N: 11-06920Inlet: 1/5'' 300RFOutlet: 2'' 150RFSet Pressure: 3.5KG/CM2G** | |  | **2** |
| **342** | **Spring  PSV MODEL: 3L4 J-JBS-E-26-KS/N: 11-06920Inlet: 1/5'' 300RFOutlet: 2'' 150RFSet Pressure: 3.5KG/CM2G** | |  | **2** |
| **343** | **Disc Holder  PSV Model: 3L4 JBS-E-26-KS/N: 11-60477INLET: 3'' 300RFOUTLET: 4'' 150RF Set Pressure: 3.5KG/CM2G** | |  | **2** |
| **344** | **Spindle  PSV Model: 3L4 JBS-E-26-KS/N: 11-60477INLET: 3'' 300RFOUTLET: 4'' 150RFSet Pressure: 3.5KG/CM2G** | |  | **2** |
| **345** | **Spring  PSV Model: 1.5 F2 JBS--E-15-KS/N: 11-06856-11-06857INLET: 1/5'' 300RFOUTLET: 2'' 150RFSet Pressure: 3.5KG/CM2G** | |  | **3** |
| **400-PSV-2002A-2002B** | | | | |
| **346** | **Disc Insert  PSV Model: 1.5G3 JBS-E32-K-SPLS/N:11-06805-11-06816Inlet: 1.5'' 300 RFOutlet: 3'' 150 RF Set Pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **347** | **Spring  PSV model: 1.5G3 JBS-E32-K-SPLS/N:11-06805-11-0680Inlet: 1.5'' 300 RFOutlet: 3'' 150 RF Set Pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **348** | **Disc Holder  PSV model: 1.5G3 JBS-E32-K-SPL S/N: 11-06815-11-06816Inlet: 1.5'' 300RFOutlet: 3'' 150RF Set Pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **FOR-400-PSV-2102A/2102B/2202A/2202B/2302A/2302B/2402A/2402B** | | | | |
| **349** | **Disc Insert  PSV MODEL: 1.5G3 JSB-E22-KInlet: 1.5'' 300RFOutlet: 3'' 150RF SET PRESSURE: 10.5KG/CM2G** | | **ROOM** | **3** |
| **350** | **Spring  PSV Model: 1.5G3 JBS-E22-KInlet: 1.5'' 300RFOutlet: 3'' 150RF Set Pressure:10.5KG/CM2G** | | **ROOM** | **3** |
| **351** | **Disc Holder  PSV Model: 1.5G3 JBS-E22-K S/N: 11-06821-11-06822Inlet: 1.5'' 300RFOutlet: 3'' 150RF Set Pressure: 10.5KG/CM2G** | | **ROOM** | **3** |
| **352** | **Bellows  PSV Model: 1.5G3 JBS-E22-KS/N: 11-06821-11-06822Inlet: 1.5'' 300RFOutlet: 3'' 150RF Set Pressure: 10.5KG/CM2G** | | **ROOM** | **3** |
| **353** | **Gasket Kit  PSV Model: 1.5G3 JBS-E32-KS/N:11-06821-11-06822Inlet: 1.5'' 300 RFOutlet: 3'' 150 RF Set Pressure: 10.5KG/CM2G** | | **ROOM** | **3** |
| **FOR-400-PSV-3501A/3501B/3601A/3601B 200-PSV-1702A-1702B** | | | | |
| **354** | **Spring  PSV Model: 3K4 JBS-E15-KS/N: 11-06879-11-06880Inlet: 3'' 150RFOutlet: 4'' 150RF Set Pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **355** | **Disc Holder  PSV Model: 3K4 JBS-E15-KS/N: 11-06879-11-06880Inlet: 3'' 150RFOutlet: 4'' 150RF Set Pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **FOR-400-PSV-4301A/4301B/4401A/4401B 200-PSV-15031/1504** | | | | |
| **356** | **Disc Insert  PSV Model: 1D2 JBS-E-15-KS/N: 11-06894-11-06895Inlet: 1'' 150RFOutlet: 2'' 150RFSet Pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **357** | **Spring  PSV Model: 1D2 JBS-E-15-KS/N: 11-06894-11-06895Inlet: 1'' 150RFOutlet: 2'' 150RFSet Pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **358** | **Disc Holder  PSV Model: 1D2 JBS-E-15-KS/N: 11-06894-11-06895Inlet: 1'' 150RFOutlet: 2'' 150RFSet Pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **359** | **Bellows  PSV Model: 1D2 JBS-E-15-KS/N: 11-06894-11-06895Inlet: 1.5'' 15RFOutlet: 2'' 150RF Set Pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **FOR-400-PSV-2910/3310** | | | | |
| **360** | **Spring  Model: 9511011E-STM S/N: 11-06859Inlet: 0.75'' 150RFOutlet: 1'' 150RFSet Pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **361** | **Spring  PSV Model: 9511011-STM S/N: 11-06859Inlet: 0.75'' 150 RFOutlet: 1'' 150 RF Set Pressure: 35KG/CM2G** | | **ROOM** | **2** |
| **362** | **Disc Holder  PSV Model: 9511011E-STM S/N: 11-06859 Inlet: 0.75'' 150RFOutlet: 1'' 150RFSet Pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **FOR-400-PSV-5118/5218** | | | | |
| **363** | **Disc Insert  PSV Model: 3J4 JBS-E-35-SK S/N: 11-06906Inlet: 3'' 300RFOutlet: 4'' 150RFSet Pressure: 31KG/CM2G** | | **ROOM** | **2** |
| **364** | **Spring  PSV Model: 3J4 JBS-E-35-SK S/N: 11-06906Inlet: 3'' 300RFOutlet: 4'' 150RFSet Pressure: 31KG/CM2** | | **ROOM** | **2** |
| **365** | **Gasket Kit  PSV Model: 3J4 JBS-E-35-SK S/N: 11-06906Inlet: 3'' 300RFOutlet: 4'' 150RFSet Pressure: 31KG/CM2** | | **ROOM** | **2** |
| **FOR-400-PSV-5103/5123/5131/5134/5142/5145** | | | | |
| **366** | **Disc Holder  PSV Model: 1D2 JBS-E-32-KS/N: 11-06901Inlet: 1'' 300RFOutlet: 2'' 150RFSet Pressure: 31KG/CM2G** | | **ROOM** | **2** |
| **367** | **Spindle  PSV Model: 1D2 JLT-JBS-E-32-KS/N: 11-06901Inlet: 1'' 300RFOutlet: 2''150RFSet Pressure: 31KG/CM2G** | | **ROOM** | **2** |
| **FOR-400-PSV-5203** | | | | |
| **368** | **Bellows  PSV Model: 1.5F2 JBS-E-35-SK S/N: 11-06906Inlet: 1.5'' 300RFOutlet: 2'' 150RF Set Pressure: 20KG/CM2G** | | **ROOM** | **1** |
| **369** | **Disc Holder  PSV Model: 1.5F2 JBS-E-35-S-KS/N: 11-06909Inlet: 1/5'' 300RFOutlet: 2'' 150RFSet Pressure: 20KG/CM2G** | | **ROOM** | **1** |
| **FOR 400-PSV-3602A/3602B** | | | | |
| **370** | **Disc Insert  PSV Model: 1.5G3 JBS-E-25-S-KS/N: 11-06881Inlet: 1.5'' 300RFOutlet: 3''150 RFSet Pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **371** | **Spring  PSV Model: 1.5G3 JBS-E-25-S-KS/N: 11-06881Inlet: 1.5'' 300RFOutlet: 3''150RFSet Pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **372** | **Gasket Kit  PSV Model: 1.5G3 JBS-E-25-S-KS/N: 11-06881Outlet:3''150RFSet Pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **373** | **Bellows Taipiece  PSV Model: 1.5G3 JBS-E-25-SK S/N: 11-06881Inlet: 1.5'' 300RFOutlet: 3'' 150RF Set Pressure: 10.5KG/CM2G** | | **ROOM** | **2** |
| **374** | **Disc Holder  PSV Model 1.5G3 JBS-E-25-S-KS/N: 11-06881Inlet: 1.5'' 300RFOutlet: 3'' 150RFSet Pressure 10.5KG/CM2G** | | **ROOM** | **2** |
| **FOR 400-PSV-5223/5231/5234** | | | | |
| **375** | **Disc Holder  PSV Model: 1D2 JBS-E-35-S-KS/N: 11-06911Inlet: 1'' 300RFOutlet: 2'' 150RFSet Pressure: 20KG/CM2G** | | **ROOM** | **2** |
| **376** | **Spring  PSV Model: 1D2 JBS-E-15-KS/N: 11-06911Inlet: 1'' 300RFOutlet: 2'' 150RFSet Pressure: 20KG/CM2G** | | **ROOM** | **2** |
| **FOR 400-PSV-5240** | | | | |
| **377** | **Bellows Taipece  PSV Model: 1E2 JBS-E-35-SK S/N: 11-06908Inlet: 1'' 300RFOutlet: 2'' 150RFSet Pressure: 23.4KG/CM2G** | | **ROOM** | **1** |
| **378** | **Disc Holder  PSV Model: 1E2 JBS-E35-S-KS/N: 11-06908Inlet: 1'' 300RFOutlet: 2'' 150 RF Set Pressure: 23.4KG/CM2G** | | **ROOM** | **1** |
| **379** | **Spring  PSV Model: 1E2 JBS-E-35-S-KS/N: 11-06908Inlet: 1'' 300 RFOutlet: 2'' 150 RF Set Pressure: 23.4KG/CM2G** | | **ROOM** | **1** |
| **FOR-400-PSV-5214** | | | | |
| **380** | **Disc Holder  PSV Model: 2H3 JBS-E-35-S-KS/N: 11-06913Inlet: 2'' 300RFOutlet: 3'' 150RFSet Pressure: 20KG/CM2G** | | **ROOM** | **1** |
| **381** | **Spring  PSV Model 2H3 JBS-E-35-S-KS/N: 11-06913Inlet: 2'' 300RFOutlet: 3'' 150RFSet Pressure: 20KG/CM2G** | | **ROOM** | **1** |
| **FOR-400-PSV-4122** | | | | |
| **382** | **Disc Holder  PSV Model: 3J4 JBS-E-32-KS/N: 11-06921Inlet: 3'' 300RFOutlet 4''150RFSet Pressure: 31KG/CM2G** | | **ROOM** | **1** |
| **383** | **Spring  PSV Model: 3J4 JBS-E-35-SK S/N: 11-06921Inlet: 3'' 300RFOutlet: 4'' 150RFSet Pressure: 31KG/CM2** | | **ROOM** | **1** |
| **384** | **Gasket Kit  Model: 3J4 JBS-E-32-k S/N: 11-06921Inlet: 3'' 300RFOutlet: 4'150RFSet Pressure: 31KG/CM2G** | | **ROOM** | **1** |
| **FOR-400-PSV-1702A~H** | | | | |
| **385** | **Spindle  PSV Model: 81PS1S6ASA-4/SPLS/N: 11-06797-11-06804Inlet: 0.75'' 150RFOutlet: 1'' 150RFSet Pressure:12.3KG/CM2G** | | **ROOM** | **3** |
| **386** | **Disc Insert  PSV Model: 81PS1S6A8A-4/SPLInlet: 0.75'' 150RFOutlet:1'' 150RF Set Pressure:12.3KG/CM2G** | | **ROOM** | **3** |
| **387** | **Spring  PSV Model: 81PS1S6A8A-4/SPLS/N: 11-06797-11-06804Inlet: 0.75'' 150RFOutlet: 1'' 150RFSet Pressure:12.3KG/CM2G** | | **ROOM** | **3** |
| **388** | **Spindle  PSV Model:81PSS6A8A-4/SPLS/N: 11-06922-11-06929Inlet: 0.75'' 150RFOutlet: 1'' 150RFSet Pressure: 9.5KG/CM2G** | | **ROOM** | **3** |
| **389** | **Disc Insert  PSV Model: 81PSS6A8A-4/SPLS/N: 11-06922-11-06929Inlet: 0.75'' 150RFOutlet:1'' 150RF Set Pressure:9.5KG/CM2G** | | **ROOM** | **3** |
| **390** | **Spring  PSV Model: 81PS1S6A8A-4/SPLS/N: 11-06922-11-06929Inlet: 0.75'' 150RFOutlet: 1'' 150RFSet Pressure: 9.5KG/CM2G** | | **ROOM** | **3** |
| **FOR-400-PSV-1301A/1301B 400-PSV-1302A/1302B** | | | | |
| **391** | **Disc Insert  PSV Model: 56605-810/S1 S/N: 11-06793-11-067986Inlet: 8'' 150RFOutlet: 10'' 150RF Set Pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **392** | **Spring  PSV Model: 56605-810/S1S/N: 11-06793-11-06796Inlet: 8'' 150RFOutlet: 10'' 150RF Set Pressure: 3.5KG/CM2G** | | **ROOM** | **2** |
| **393** | **O.Ring Kit  Model: 56605-810/S1S/N: 11-067** | | **Room** | **2** |
| **PDR FOR PSV VALVE MODEL 45312D12/S1 UNIT 1081-700-701-100** | | | | |
| **394** | **Seal  Model PSV 45312D12/S1N°7 on drawingConst: TYCO** | | **ROOM** | **8** |
| **PDR FOR PSV TYCO** | | | | |
| **395** | **Spring  Description: SPR SPRING- FREE LGTH 11.50 ODMAX 5.20 COP/n: X36269 Const: TYCO** | | **ROOM** | **2** |
| **PDR FOR VALVE PSV 3J4 JOS-E-35-E UNIT: 701-703-1091** | | | | |
| **396** | **Disc holder  PSV MODEL No.: 3J4 JOS-E-35-EConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 1E2 JOS-E-25-E UNIT: 701-703-1091** | | | | |
| **397** | **Disc holder  PSV MODEL No.: 1E2 JOS-E-25-EConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 3K4 JLT-JBS-E-15-K UNIT: 31-11-10-700** | | | | |
| **398** | **Disc holder  PSV MODEL No.: 3K4 JLT-JBS-E-15-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 4N6 JBS-15-N2-K UNIT: 31-11-10-700** | | | | |
| **399** | **Disc holder  PSV MODEL No.: 4N6 JBS-15-N2-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 3J4 JOS-E-35-E UNIT: 701-703-1091** | | | | |
| **400** | **Disc holder  PSV MODEL N°: 2J3 JLT-JBS-E-25-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 1,5H3 JBS-E-15-K UNIT: 1081-700-701-100** | | | | |
| **401** | **Disc holder  PSV MODEL No.: 1.5H3 JBS-E-15-K Const: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 3J4 JBS-E-15-K UNIT: 1081-700-701-100** | | | | |
| **402** | **Disc holder  PSV MODEL No.: 3J4 JBS-E-15-KConst: TYCO** | | **ROOM** | **6** |
| **PDR FOR VALVE PSV 4M6 JBS-E-15-K UNIT: 701-703-1091** | | | | |
| **403** | **Disc holder  PSV MODEL N°: 4M6 JBS-E-15-KConst: TYCO** | | **ROOM** | **6** |
| **P/Automatic Valve Mod: 2P 05 Type Globe Post Size 3B x 3B CV 125-LIFT 38 MM IPI 3000RF** | | | | |
| **404** | **Positioner  Mod: AO-700 DInpit Singnal 0.2÷1KG/CM2** | | **ROOM** | **2** |
| **PDR Valve PSV JNO 15S1-C UNIT:1051/1061** | | | | |
| **405** | **Disc Holder  PSV Model No.: JNO-15S1-C** | | **ROOM** | **9** |
| **406** | **Spring  Model: 9511012B-SPL** | | **ROOM** | **9** |
| **407** | **Gasket Cap Top  PSV Model No.: JNO-15S1-C** | | **ROOM** | **9** |
| **408** | **Gasket Cap Top  PSV Model No.: JNO-15S1-C** | | **ROOM** | **9** |
| **PDR For PSV Valve No. JLT-JNO-15S1-B UNIT: 1061-1022** | | | | |
| **409** | **Disc Holder  N°06 on DrawingVale PSV N° JLT-JNO-15S-B** | | **ROOM** | **23** |
| **410** | **Spring  N°11 on drawingVale PSV N° JLT-JNO-15S-B** | | **ROOM** | **23** |
| **411** | **Gasket Cap Top  N°30 on drawingPSV Model N°: JLT-JNO-15S1-B** | | **ROOM** | **23** |
| **412** | **Gasket CAP  N°32 On drawingVale PSV N° JLT-JNO-15S-B** | | **ROOM** | **23** |
| **For Vale PSV - Model No. JON-16S1** | | | | |
| **413** | **Disc Holder  N°6 On drawing** | | **ROOM** | **8** |
| **414** | **Spring  N°11 on drawing** | | **ROOM** | **8** |
| **415** | **Disc Holder  N°06 on DrawingVale PSV N° JLT-JNO-15S-B** | | **ROOM** | **8** |
| **416** | **Spring  N°11 on drawingVale PSV N° JLT-JNO-15S-B** | | **ROOM** | **8** |
| **417** | **Gasket Cap Top  N°30 on drawingPSV Model N°: JLT-JNO-15S-B** | | **ROOM** | **8** |
| **418** | **Gasket CAP  N°32 On drawingVale PSV N° JLT-JNO-15S-B** | | **ROOM** | **8** |
| **P/Safety valves** | | | | |
| **419** | **Nozzle P/Valve  Mod JNO-H-47-SSize 4P6-MAT.ASTM A182 GRF 316Serie No. C.95540** | | **ROOM** | **2** |
| **420** | **Nozzle P/Valve  Mod JNO-H-25-S1Size 2J3-MAT.ASTM A182 GRF 316Serie No. C.9379** | | **ROOM** | **2** |
| **421** | **Nozzle For Valve  Mod: JNO/JNB-35-S1-BSize 1 1/2 F2** | | **ROOM** | **1** |
| **422** | **Nozzle For Valve  Mod: JNO/JNB H-35-S1Size 4L6  Mat . A 351 CF 8M/A 182F3-SERIE N°C93025** | | **ROOM** | **18** |
| **423** | **Bellows  Ref. 2H3''Mat.SUS 316C** | | **ROOM** | **2** |
| **424** | **Nozzle P/Valve  Mod.JNB/JNO 35 S1 B/CSize 2H3 MAT.ASTM A 192 GRF 316SERIE C93036** | | **ROOM** | **2** |
| **425** | **Spring P/ Valve  Ref.6073 DIM. 11/2 F.2Type.JNO.35.51.BSet DE TRAGE SRG/CM2** | | **ROOM** | **1** |
| **P/Safety Valve Mod: JNB-35-MH-E S/N C93009-1''300 RFXDX 2'' 150 RF** | | | | |
| **426** | **Valve  Ref: 1D2''Mat: Monel K500** | | **ROOM** | **1** |
| **427** | **Valve  Dim: 1 1/2 2''Mat: ASTM A 182 GRF 316** | | **ROOM** | **2** |
| **428** | **Nozzle  Model: HS 26 S1 Siez: 2J3Mat ASTM A 182 GRF 316 Serial No.: C93026** | | **ROOM** | **1** |
| **429** | **Spring P/Valve  Rep: 6471Dim: 21 1/2 J4Type JND 35.S1B Calibration set: 18 KG/Cm2 Qra-AD** | | **ROOM** | **1** |
| **430** | **Spring P/Valve  Dim 3/4 W1Dim: 21 1/2 J4Type JMB.C.SXB Setting pressure: 18 KG/Cm2 Qra-AD** | | **ROOM** | **1** |
| **431** | **Steel gasket  Rep: 1 1/2'' G 2 1/2''Mat V560 (S10C)** | | **ROOM** | **2** |
| **432** | **Spring P/Valve  Ref: 6205 Dim: 4L6** | | **ROOM** | **1** |
| **P/ Safety valve** | | | | |
| **433** | **Nozzle P/Valve  Mod HS.25.S1 Size 3M6Mat: ASTM A 182 GRF 316Serie N°: C.93021** | | **ROOM** | **2** |
| **434** | **Steel seal  Dim: 2H3Mat V560 (S10L )  Ref: 11/2F'' N°REF: 2H3** | | **ROOM** | **10** |
| **435** | **Nozzle P/Valve  Model: JNO 36 M1 E Size: 4L6Mat: Monel K 500Series n°: C93001** | | **ROOM** | **2** |
| **P/ Safety valve Mat: Monel.K.500 Serial: n°C 93013 QRA/02** | | | | |
| **436** | **Nozzle P/Valve  Mod: JNB 35 M1 E; JNB 36 M1 ESize: 6 Q 8Mat: Monel K 500Series: n° C 93013 QRA/02** | | **ROOM** | **1** |
| **437** | **Nozzle P/Valve  Mod JNO.H 35-SDim: 1'' 1/2 H3Series N°: C 93033Mat: ASTM A 182 GRF 316** | | **ROOM** | **1** |
| **P/ Safety valve Mod: JNB-35-M1-E S/N°:C93013-103-PSV-108** | | | | |
| **438** | **Bellows  Ref. SL-03089-01-3503Mat.SUS 316L** | | **ROOM** | **2** |
| **439** | **Spring P/Valve  Ref: 6211 Dim: 4L6Type JNO 35 S1 BSet of calibration: 16.5kg/cm2** | | **ROOM** | **1** |
| **440** | **Nozzle P/valve  Mod JNO 35 S1 BSize 4L6 Mat,ASTM A 531 CF 8M/A 182F3Serie C93042** | | **ROOM** | **1** |
| **441** | **Nozzle P/ Valve  Mod. JLT.JNB 25.SX.B and 25 S1.B Size 2J3Mat. ASTM A 182 GRF 316  Series No. C 93039** | | **ROOM** | **2** |
| **442** | **Valve  Ref: 4K''Mat: Monel K500** | | **ROOM** | **1** |
| **443** | **Valve  Ref: 2J3 A20-56-02Mat.ASTM A 182 GRF 316** | | **ROOM** | **2** |
| **444** | **Valve  Ref: 4P6Mat: ASTM A 182 GRF 316** | | **ROOM** | **2** |
| **445** | **Spring P/Valve  Ref: 1043 , Type JMB.C.SXB  DIM: 3/4 W1 Setting pressure: 20.9 KG/CM2** | | **ROOM** | **6** |
| **446** | **Spring P/Valve  Ref: 1095Mat: JMB.C.SX.B/ DIM: 3/4 W1Setting pressure: 6KG/CM2** | | **ROOM** | **14** |
| **447** | **Spring P/Valve  Dim 4PC REF 6816Type J.N0 H.47.S1String set: 36KG/CM2** | | **ROOM** | **2** |
| **448** | **Spring For Valve  Ref 6304-DIM: 6Q8Type J.N0 H.25.S1Set of 6KG/CM2** | | **ROOM** | **2** |
| **449** | **Spring P/Valve  Ref 6054-DIM: 2J3Type J.N0 H.25.S1Set of calibration: 6KG/CM2** | | **ROOM** | **2** |
| **450** | **Spring P/Valve  Ref 1107 Type: JMB.C.SXBDim 3/4 W1Taring set 1.4 KG/CM2** | | **ROOM** | **1** |
| **451** | **Spring For Valve  Ref 1402Type JMB.C.SXBDIM 3/4 W1/ SETDE: Taring 13.9KG CM2** | | **ROOM** | **1** |
| **P/ Safety valve** | | | | |
| **452** | **Spring For valve  Ref/6092 DIM 11/2 G.2 1/2Type JNO.35.M1.EStaring set: 43KG/CM2** | | **ROOM** | **2** |
| **453** | **Spring For Valve  Dim: 2J3Ref 7061Type JLT.JNB 25.SX.BTaring set 18.5 KG** | | **ROOM** | **1** |
| **454** | **Spring P/Valve  Ref 6081-DIM 2H3Type JNB 35 S1 BSet of trage 11KG/CM2** | | **ROOM** | **1** |
| **455** | **Spring P/Valve  Ref 6093-DIM 2H3Type JNO 35 S1 BSet of calibration 36KG/CM2** | | **ROOM** | **1** |
| **456** | **Spring For Valve  Dim: 1E2 REF.6014Type JNO H 35 S Calibration set 6KG/CM2** | | **ROOM** | **1** |
| **457** | **Spring For Valve  Type: HS 25-S1Dim: 3 m 6Ref: Q 1159Setting pressure: 36KG/CM2** | | **ROOM** | **1** |
| **458** | **Spring for valve  Ref: 6077Type: JNO H 25-S1Dim: 1'' 1/2 H3Taring set= 6 KG/CM2** | | **ROOM** | **2** |
| **459** | **Nozzel P/Valve  Mod: JMB-C-SXB SiZE 3/4 W1Mat: ASTM.A.182.GRF316SERIE: N°C93007** | | **ROOM** | **20** |
| **460** | **Nozzle P/VALVE  MOD: JNO 35 ME1E JNB 36 M1 ESIZE:2H3 MAT: MONEL.K.500Serie N° C93017** | | **ROOM** | **1** |
| **461** | **Nozzle  MOD: JNO.35.M1.ESIZE 1 E2 MAT: MONEL.K.500SERIE N°C.93005** | | **ROOM** | **2** |
| **462** | **Nozzle P/Valve  MOD: JNO.H.35.S1Mat: ASTM A18GRF316SERIE: C93023** | | **ROOM** | **1** |
| **463** | **Nozzle P/Valve  MOD.JNO-H-25-S1Size 6-Q8 MAT,ASTM A 351 CF 8M/A 182 F3SERIE C93073** | | **ROOM** | **2** |
| **464** | **Valve  Ref: 2J3'' 38425Mat.ASTM A 182 GRF 316** | | **ROOM** | **2** |
| **465** | **Spring P/Valve  Type: H.S26.S1Ref: T 573Dim: 2J3 Pulling pressure 34 kg/cm2** | | **ROOM** | **2** |
| **PDR Valve PSV JNO 15S1-C UNIT:1051/1061** | | | | |
| **466** | **Disc Insert  Model No.: JNO-15S1-C** | | **ROOM** | **9** |
| **467** | **Disc Insert  No. 03 on drawingVale PSV No. JLT-JNO-15S-B** | | **ROOM** | **8** |
| **PDR FOR PSV VALVE N°JLT-JNO-15S1-B UNIT: 1061-1022** | | | | |
| **468** | **Disc Insert  No. 03 on drawingVale PSV No. JLT-JNO-15S1-B** | | **ROOM** | **23** |
| **469** | **Disc Insert  N°03 on drawing** | | **ROOM** | **8** |
| **P/SAFETY VALVE** | | | | |
| **470** | **Nozzle f/valve  Mod: JNB-35-M1-ESize: 3K4 Mat: MONEL K 500Serie N°: C 93015** | | **ROOM** | **2** |
| **PDR for safety valve  type REC 261 Dim: 3" 300 x 4" 150, series 3 x K x 4 103, Fluid: C3H8, pressure: 18Kg/Cm2** | | | | |
| **Serial No. 013328** | | | | |
| **471** | Gasket (seal):  REP: 25MAT: aramid fiber | | PS | 2 |
| **472** | Gasket (seal):  REP: 27MAT: aramid fiber | | PS | 2 |
| **Serial No. 013329 and 013331** | | | | |
| **473** | Spring:  REP: 13 SUP: 9 | | PS | 1 |
| **474** | Disc:  REP: 2 SUS: 304 | | PS | 1 |
| **475** | Nozzle (nose):  REP: 1 SUS: 304 | | PS | 1 |
| **PDR for safety valve  type REC 261, Dim 11/2 "300 x 3" 150, series 1-1/2 x H x 3 103 , Fluid : C3H8, pressure: 18Kg/Cm2** | | | | |
| **Serial No. 013329 and 013331** | | | | |
| **476** | Gasket (seal):  REP: 25Mat: aramid fiber | | PS | 2 |
| **477** | Gasket (seal)  REP: 26 Mat : aramid fiber | | PS | 2 |
| **480** | Gasket (seal):  REP: 27 Mat: aramid fiber | | PS | 2 |
| **481** | Spring (spring):  REP: 26 REF: SUP 9 | | PS | 1 |
| **482** | Disc:  REP: 2 REF: SUS: 304 | | PS | 1 |
| **483** | Nozzle (nose):  REP: 1 REF: SUS: 304 | | PS | 1 |
| **PDR for safety valve  type REC 261, Dim 11/2 "300 x 3" 150, series 2 x J x 3 103, Fluid: C3H8, pressure: 18Kg/Cm2 Serial No. 013330** | | | | |
| **484** | Gasket (seal):  REP: 25MAT: aramid fiber | | PS | 2 |
| **485** | Gasket (seal):  REP: 27MAT: aramid fiber | | PS | 2 |
| **486** | Spring (spring):  REP: 13 REF: SUP 9 | | PS | 1 |
| **487** | Disc (disc):  REP: 2 REF: SUS 304 | | PS | 1 |
| **488** | Nozzle (nose):  REP: 1 REF: SUS 304 | | PS | 1 |
| **PSV MODEL SL431-M** | | | | |
| **489** | SPRING #16 ON DRAWING | | PS | 3 |
| **490** | SPINDLE N° 07 ON DRAWING | | PS | 3 |
| **491** | DISC HOLDER N° 05 ON DRAWING | | PS | 3 |
| **492** | GASKET KIT | | PS | 3 |
| **494** | DISC N° 02 ON DRAWING | | PS | 3 |
| **PSV MODEL SL131** | | | | |
| **494** | SPRING #16 ON DRAWING | | PS | 4 |
| **495** | SPINDLE N° 07 ON DRAWING | | PS | 4 |
| **496** | DISC HOLDER N° 03 ON DRAWING | | PS | 4 |
| **four hundred ninety seven** | GASKET KIT | | PS | 4 |
| **498** | DISC N° 02 ON DRAWING | | PS | 4 |
| **PSV MODEL SL431-M2** | | | | |
| **499** | SPRING #16 ON DRAWING | | PS | 3 |
| **500** | SPINDLE N° 07 ON DRAWING | | PS | 3 |
| **501** | DISC HOLDER N° 05 ON DRAWING | | PS | 3 |
| **502** | GASKET KIT | | PS | 3 |
| **503** | DISC N° 02 ON DRAWING | | PS | 3 |
| **For the substitution of the ( 1051 -PSV-1325)** | | | | |
| **504** | Back Pressure  Valve VSM 11/2'' AISI 150 SET.P.2KG/CM2Brand: Seko | | PS | 1 |
| **PDR for safety valves type model: 1D2 JBS-E-36-SPL TYPE K**  **TAG: 100-PSV-1501A/1501B/1502A Set pressure: 27 KG/CM2 SN° 11-05676**  **DWG: DS 108-4869** | | | | |
| **505** | Disc Insert MTL  ASME SA479 Type 316 PSV Model: 1D2 JBS-E-36-SPL TYPE K  Set pressure: 27 KG/CM2 SN° 11-05676  Item: 08 DWG: DS 108-4869 | | PS | 1 |
| **506** | Disc Holder  MTL: 316L SST PSV Model: 1D2 JBS-E-36-SPL TYPE K  Set pressure: 27 KG/CM2 SN° 11-05676  Item: 05 DWG: DS 108-4869 | | PS | 1 |
| **Valve needed for running reforming unit II (103-PSV-322)** | | | | |
| **507** | A complete TARE A 6 KG/CM2G safety valve with calibration certificate S/N NO: C96457 Requires  a nameplate with the following data :  TAG N°: 103-PSV-322Model: JNO-H-35 S1S/R NO: C96457Dimension: 2'' 300#RF X 3'' 150#RFOrifice: 2 XHX 3Set pressure: 6 KG/CM2GFluid: LP steam | PS | 1 | |
| **Valve needed for running reforming unit II (103-PSV-312)** | | | | |
| **508** | A complete TARE A 6 KG/CM2G safety valve with calibration certificate S/N NO: C93025 Requires  a nameplate with the following data :  TAG N°: 103-PSV-312Model: JNO-H-35 S1S/R NO: C93025Dimension: 4'' 300#RF X 6'' 150#RFOrifice: 4 XLX 6Set pressure: 6 KG/CM2GFluid: LP steam | PS | 1 | |
| **Valve needed for running reforming unit II (103-PSV-311B)** | | | | |
| **509** | A complete TARE A 6 KG/CM2G safety valve with calibration certificate S/N NO: C93024 Requires  a nameplate with the following data :  TAG N°: 103-PSV-311BModel: JNO-H-35 S1S/R NO: C93024Dimension: 1'' 300#RF X 2'' 150#RFOrifice: 1 XEX 2Set pressure: 6 KG/CM2GFluid: LP steam | PS | 1 | |
| **P/ Safety valve** | | | | |
| **510** | Spring P/Valve  Dim: 2H3 REF: 6077Type: JNO. H35-S1  Taring set: 6KG/CM2 | PS | 2 | |
| **511** | Nozzle P/Valve  Dim: 2H3 Mod: JNO. H35-S1  Matt: ASTM A182GRF316 Series No.: C96457 | PS | 1 | |